{"text_format":"1","workbook":"xlsx","n_sheets":7,"sheets":["Vurdering af miljøgevinst","Ruteoplysninger","Brændstoftyper","Emissionspriser","Andre tiltag","Brændstofforbrug","Diverse"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":30991,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Vurdering af miljøgevinst","index":0,"n_rows":4392,"n_cols":6,"rows_kept":4392,"cut":false,"hidden":false,"merged":[[15,0,15,1],[3,0,3,1],[65,0,65,1]]}
[]
[]
[]
["VALG AF PARAMETRE"]
["Rute 1","Tiltag",null,null,"Rute 1","Sammenligningsgrundlag"]
["Brændstoftype","Biodiesel",null,null,"Brændstoftype","Diesel"]
["Euro-norm","Euro 6",null,null,"Euro-norm","Euro 3"]
["Buslængde","12 meter",null,null,"Buslængde","12 meter"]
["Brændstofforbrug i km/liter eller ved gas i km/NM3",3.1814129686297981,null,null,"Brændstofforbrug i km/liter eller ved gas i km/NM3",2.6181579395801373]
["Økochaufførkursus","Ja",null,null,"Økochaufførkursus","Nej"]
["Ekstra partikelfilter","Ja",null,null,"Ekstra partikelfilter","Nej"]
["Brændstofbesparelse pr. km",0,null,null,"Brændstofbesparelse pr. km",0]
["Ved biodiesel eller ethanol vælg blandingsforhold",0.35,null,null,"Ved biodiesel eller ethanol vælg blandingsforhold",0]
[]
[]
["RESULTAT FOR SAMLEDE RUTER"]
["Estimerede emissioner (tiltag)","I gram","I kroner","Estimerede emissioner (sammenligningsgrundlag)","I gram","I kroner"]
["Kuldioxid (CO2)",{"$f":"Emissioner_rute1_1_kul","v":57322435.596452378},{"$f":"Pris_rute1_1_kul","v":7451.9166275388097},"Kuldioxid (CO2)",{"$f":"Emissioner_rute1_2_kul","v":120405264.79871328},{"$f":"Pris_rute1_2_kul","v":15652.684423832728}]
["Svovldioxid (SO2)",{"$f":"Emissioner_rute1_1_svovl","v":425.5916744072199},{"$f":"Pris_rute1_1_svovl","v":88.842262032507165},"Svovldioxid (SO2)",{"$f":"Emissioner_rute1_2_svovl","v":813.54908647779246},{"$f":"Pris_rute1_2_svovl","v":169.82837180223919}]
["Kvælstofilter (NOX)",{"$f":"Emissioner_rute1_1_kvæl","v":26580.846382989726},{"$f":"Pris_rute1_1_kvæl","v":1275.880626383507},"Kvælstofilter (NOX)",{"$f":"Emissioner_rute1_2_kvæl","v":474570.30044537887},{"$f":"Pris_rute1_2_kvæl","v":22779.374421378187}]
["Kultile (CO)",{"$f":"Emissioner_rute1_1_kulilt","v":99678.173936211489},{"$f":"Pris_rute1_1_kulilt","v":1.6446898699474894},"Kulilte (CO)",{"$f":"Emissioner_rute1_2_kulilt","v":199319.52618705915},{"$f":"Pris_rute1_2_kulilt","v":3.2887721820864759}]
["Kulbrinte (HC)",{"$f":"Emissioner_rute1_1_kulbrint","v":8638.7750744716632},{"$f":"Pris_rute1_1_kulbrint","v":23.756631454797077},"Kulbrinte (HC)",{"$f":"Emissioner_rute1_2_kulbrint","v":62643.279658790023},{"$f":"Pris_rute1_2_kulbrint","v":172.26901906167257}]
["Partikler (PM)",{"$f":"Emissioner_rute1_1_part","v":49.839086968105725},{"$f":"Pris_rute1_1_part","v":61.252237883801939},"Partikler (PM)",{"$f":"Emissioner_rute1_2_part","v":9491.4060089075792},{"$f":"Pris_rute1_2_part","v":11664.937984947415}]
["Samlede miljøomkostninger for tiltag",null,{"$f":"SUM(Sumpris_kul_tiltag:C23)","v":8903.2930751633703},"Samlede miljøomkostninger for sammenligningsgrundlag",null,{"$f":"SUM(Sumpris_kul_sammenligning:Sumpris_part_sammenligning)","v":50442.382993204323}]
[]
[]
["Estimerede emissionbesparelser","I gram","I procent","Estimerede emissionsbesparelser (kroner)","I kroner"]
[{"$f":"D18","v":"Kuldioxid (CO2)"},{"$f":"(Sum_kul_sammenligning-Sum_kul_tiltag)","v":63082829.202260904},{"$f":"IF(Sum_kul_sammenligning=0,\"Kan ikke udregnes\",(Sum_kul_sammenligning-Sum_kul_tiltag)/Sum_kul_sammenligning)","v":0.52392085435565638},"Kuldioxid (CO2)",{"$f":"Sumpris_kul_sammenligning-Sumpris_kul_tiltag","v":8200.7677962939197}]
["Svovldioxid (SO2)",{"$f":"(Sum_svovl_sammenligning-Sum_svovl_tiltag)","v":387.95741207057256},{"$f":"IF(Sum_svovl_sammenligning=0,\"Kan ikke udregnes\",(Sum_svovl_sammenligning-Sum_svovl_tiltag)/Sum_svovl_sammenligning)","v":0.47687031860635332},"Svovldioxid (SO2)",{"$f":"Sumpris_svovl_sammenligning-Sumpris_svovl_tiltag","v":80.986109769732025}]
["Kvælstofilter (NOX)",{"$f":"(Sum_kvæl_sammenligning-Sum_kvæl_tiltag)","v":447989.45406238915},{"$f":"IF(Sum_kvæl_sammenligning=0,\"Kan ikke udregnes\",(Sum_kvæl_sammenligning-Sum_kvæl_tiltag)/Sum_kvæl_sammenligning)","v":0.94398965472967045},"Kvælstofilter (NOx)",{"$f":"Sumpris_kvæl_sammenligning-Sumpris_kvæl_tiltag","v":21503.49379499468}]
["Kulilte (CO)",{"$f":"(Sum_kulilt_sammenligning-Sum_kulilt_tiltag)","v":99641.35225084766},{"$f":"IF(Sum_kulilt_sammenligning=0,\"Kan ikke udregnes\",(Sum_kulilt_sammenligning-Sum_kulilt_tiltag)/Sum_kulilt_sammenligning)","v":0.49990763151491424},"Kulilte (CO)",{"$f":"Sumpris_kulilt_sammenligning-Sumpris_kulilt_tiltag","v":1.6440823121389865}]
["Kulbrinte (HC)",{"$f":"(Sum_kulbrint_sammenligning-Sum_kulbrint_tiltag)","v":54004.504584318362},{"$f":"IF(Sum_kulbrint_sammenligning=0,\"Kan ikke udregnes\",(Sum_kulbrint_sammenligning-Sum_kulbrint_tiltag)/Sum_kulbrint_sammenligning)","v":0.86209574081168849},"Kulbrinte (HC)",{"$f":"Sumpris_kulbrint_sammenligning-Sumpris_kulbrint_tiltag","v":148.51238760687548}]
["Partikler (PM)",{"$f":"(Sum_part_sammenligning-Sum_part_tiltag)","v":9441.5669219394731},{"$f":"IF(Sum_part_sammenligning=0,\"Kan ikke udregnes\",(Sum_part_sammenligning-Sum_part_tiltag)/Sum_part_sammenligning)","v":0.99474903013090654},"Partikler (PM)",{"$f":"Sumpris_part_sammenligning-Sumpris_part_tiltag","v":11603.685747063613}]
[null,null,null,"Total årlig  miljøbesparelse",{"$f":"SUM(Sumpris_besparelse_kul:Sumpris_besparelse_part)","v":41539.089918040961}]
[null,null,null,"Miljøindeks for tiltag",{"$f":"IF(Samlede_miljøomkostninger_sammenligning=0,\"Kan ikke udregnes\",Samlede_miljøomkostninger_tiltag*100/Samlede_miljøomkostninger_sammenligning)","v":17.650421226853688}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["RESULTAT FOR ENKELTE RUTER"]
["Rute 1"]
["Årligt brændstofforbrug for tiltag",{"$f":"IF(Brændstof=\"El\",\"Ikke oplyst\",IF(Okochau=\"Ja\",AntalKM/Forbrug*(1-Bbesparelse)*(1-OkoVærdi),AntalKM/Forbrug*(1-Bbesparelse)))","v":33569.989515066838},{"$f":"IF(Brændstof=\"Diesel\",\"Liter\",IF(Brændstof=\"Biodiesel\",\"Liter\",IF(Brændstof=\"Naturgas\",\"NM(3)\",IF(Brændstof=\"Biogas\",\"NM(3)\",IF(Brændstof=\"Ethanol\",\"Liter\",IF(Brændstof=\"El\",\"\",IF(Brændstof=\"Brint\",\"NM(3)\",\"Fejl\")))))))","v":"Liter"}]
["Årligt brændstofforbrug for sammenligningsgrundlag",{"$f":"IF(Brændstof2=\"El\",\"Ikke oplyst\",IF(Okochau2=\"Ja\",AntalKM/Forbrug2*(1-Bbesparelse2)*(1-OkoVærdi),AntalKM/Forbrug2*(1-Bbesparelse2)))","v":45833.751350861545},{"$f":"IF(Brændstof2=\"Diesel\",\"Liter\",IF(Brændstof2=\"Biodiesel\",\"Liter\",IF(Brændstof2=\"Naturgas\",\"NM(3)\",IF(Brændstof2=\"Biogas\",\"NM(3)\",IF(Brændstof2=\"Ethanol\",\"Liter\",IF(Brændstof2=\"El\",\"\",IF(Brændstof2=\"Brint\",\"NM(3)\",\"Fejl\")))))))","v":"Liter"}]
["Årlig brændstofbesparelse ved gennemførelse af tiltag",{"$f":"IF(OR(Brændstof=\"El\",Brændstof2=\"El\"),\"Ikke oplyst\",IF(Rute1_enhed1=Rute1_enhed2,Rute1_brændstofforbrug_sammenligning-Rute1_brændstofforbrug_tiltag,\"Enheder ikke sammenlignelige\"))","v":12263.761835794707},{"$f":"IF(Rute1_enhed1=Rute1_enhed2,Rute1_enhed2,\"\")","v":"Liter"}]
["Årligt effektivt energiforbrug for tiltag",{"$f":"IF(Brændstof=\"Diesel\",Rute1_brændstofforbrug_tiltag*Brændstoftyper!B14,IF(Brændstof=\"Biodiesel\",Rute1_brændstofforbrug_tiltag*Diverse!B4,IF(Brændstof=\"Naturgas\",Rute1_brændstofforbrug_tiltag*Brændstoftyper!D14,IF(Brændstof=\"Biogas\",Rute1_brændstofforbrug_tiltag*Brændstoftyper!E14,IF(Brændstof=\"Ethanol\",Rute1_brændstofforbrug_tiltag*Diverse!C4,\"Ikke oplyst\")))))","v":1139179.1306995598},"MJ"]
["Årligt effektivt energiforbrug for sammenligningsgrundlag",{"$f":"IF(Brændstof2=\"Diesel\",Rute1_brændstofforbrug_sammenligning*Brændstoftyper!B14,IF(Brændstof2=\"Biodiesel\",Rute1_brændstofforbrug_sammenligning*Diverse!D4,IF(Brændstof2=\"Naturgas\",Rute1_brændstofforbrug_sammenligning*Brændstoftyper!D14,IF(Brændstof2=\"Biogas\",Rute1_brændstofforbrug_sammenligning*Brændstoftyper!E14,IF(Brændstof2=\"Ethanol\",Rute1_brændstofforbrug_sammenligning*Diverse!E4,\"Ikke oplyst\")))))","v":1627098.1729555849},"MJ"]
["Årlig  effektiv energibesparelse",{"$f":"IF(AND(ISNUMBER(Rute1_energiforbrug_tiltag),ISNUMBER(Rute1_energiforbrug_sammenligning)),Rute1_energiforbrug_sammenligning-Rute1_energiforbrug_tiltag,\"Ikke oplyst\")","v":487919.04225602513},{"$f":"IF(ISNUMBER(Rute1_energibesparelse),\"MJ\",\"\")","v":"MJ"}]
[]
[]
["Estimerede emissioner (tiltag)","I gram","I kroner","Estimerede emissioner (sammenligningsgrundlag)","I gram","I kroner"]
["Kuldioxid (CO2)",{"$f":"Rute1_brændstofforbrug_tiltag*Diverse!$H$4","v":57322435.596452378},{"$f":"(Emissioner_rute1_1_kul*Emissionspriser!$B$21*AndelBy+Emissioner_rute1_1_kul*Emissionspriser!$B$20*(1-AndelBy))/1000","v":7451.9166275388097},"Kuldioxid (CO2)",{"$f":"Rute1_brændstofforbrug_sammenligning*Diesel_Euro3_kul","v":120405264.79871328},{"$f":"(Emissioner_rute1_2_kul*Emissionspriser!$B$21*AndelBy+Emissioner_rute1_2_kul*Emissionspriser!$B$20*(1-AndelBy))/1000","v":15652.684423832728}]
["Svovldioxid (SO2)",{"$f":"Rute1_brændstofforbrug_tiltag*Diverse!$H$5","v":425.5916744072199},{"$f":"(Emissioner_rute1_1_svovl*Emissionspriser!$G$21*AndelBy+Emissioner_rute1_1_svovl*Emissionspriser!$G$20*(1-AndelBy))/1000","v":88.842262032507165},"Svovldioxid (SO2)",{"$f":"Rute1_brændstofforbrug_sammenligning*Diesel_Euro3_svovl","v":813.54908647779246},{"$f":"(Emissioner_rute1_2_svovl*Emissionspriser!$G$21*AndelBy+Emissioner_rute1_2_svovl*Emissionspriser!$G$20*(1-AndelBy))/1000","v":169.82837180223919}]
["Kvælstofilter (NOx)",{"$f":"Rute1_brændstofforbrug_tiltag*Diverse!$H$6","v":26580.846382989726},{"$f":"(Emissioner_rute1_1_kvæl*Emissionspriser!$D$21*AndelBy+Emissioner_rute1_1_kvæl*Emissionspriser!$D$20*(1-AndelBy))/1000","v":1275.880626383507},"Kvælstofilter (NOx)",{"$f":"Rute1_brændstofforbrug_sammenligning*Diesel_Euro3_kvæl","v":474570.30044537887},{"$f":"(Emissioner_rute1_2_kvæl*Emissionspriser!$D$21*AndelBy+Emissioner_rute1_2_kvæl*Emissionspriser!$D$20*(1-AndelBy))/1000","v":22779.374421378187}]
["Kulilte (CO)",{"$f":"Rute1_brændstofforbrug_tiltag*Diverse!$H$7","v":99678.173936211489},{"$f":"(Emissioner_rute1_1_kulilt*Emissionspriser!$E$21*AndelBy+Emissioner_rute1_1_kulilt*Emissionspriser!$EB$20*(1-AndelBy))/1000","v":1.6446898699474894},"Kulilte (CO)",{"$f":"Rute1_brændstofforbrug_sammenligning*Diesel_Euro3_kulilt","v":199319.52618705915},{"$f":"(Emissioner_rute1_2_kulilt*Emissionspriser!$E$21*AndelBy+Emissioner_rute1_2_kulilt*Emissionspriser!$EB$20*(1-AndelBy))/1000","v":3.2887721820864759}]
["Kulbrinte (HC) ",{"$f":"Rute1_brændstofforbrug_tiltag*Diverse!$H$8","v":8638.7750744716632},{"$f":"(Emissioner_rute1_1_kulbrint*Emissionspriser!$F$21*AndelBy+Emissioner_rute1_1_kulbrint*Emissionspriser!$F$20*(1-AndelBy))/1000","v":23.756631454797077},"Kulbrinte (HC) ",{"$f":"Rute1_brændstofforbrug_sammenligning*Diesel_Euro3_kulbrint","v":62643.279658790023},{"$f":"(Emissioner_rute1_2_kulbrint*Emissionspriser!$F$21*AndelBy+Emissioner_rute1_2_kulbrint*Emissionspriser!$F$20*(1-AndelBy))/1000","v":172.26901906167257}]
["Partikler (PM)",{"$f":"(Rute1_brændstofforbrug_tiltag*Diverse!$H$9)*PFværdi","v":49.839086968105725},{"$f":"(Emissioner_rute1_1_part*Emissionspriser!$C$21*AndelBy+Emissioner_rute1_1_part*Emissionspriser!$C$20*(1-AndelBy))/1000","v":61.252237883801939},"Partikler (PM)",{"$f":"Rute1_brændstofforbrug_sammenligning*Diesel_Euro3_part","v":9491.4060089075792},{"$f":"(Emissioner_rute1_2_part*Emissionspriser!$C$21*AndelBy+Emissioner_rute1_2_part*Emissionspriser!$C$20*(1-AndelBy))/1000","v":11664.937984947415}]
["Samlede årlige miljøomkostninger for tiltag",null,{"$f":"SUM(Pris_rute1_1_kul:Pris_rute1_1_part)","v":8903.2930751633703},"Samlede årlige miljøomkostninger for sammenligningsgrundlag",null,{"$f":"SUM(Pris_rute1_2_kul:Pris_rute1_2_part)","v":50442.382993204323}]
["Estimerede emissionsbesparelser for rute 1","I gram","I procent","Estimerede emissionsbesparelser for rute 1","I kroner"]
["Kuldioxid (CO2)",{"$f":"Emissioner_rute1_2_kul-Emissioner_rute1_1_kul","v":63082829.202260904},{"$f":"IF(Emissioner_rute1_2_kul=0,\"Kan ikke udregnes\",(Emissioner_rute1_2_kul-Emissioner_rute1_1_kul)/Emissioner_rute1_2_kul)","v":0.52392085435565638},"Kuldioxid (CO2)",{"$f":"Pris_rute1_2_kul-Pris_rute1_1_kul","v":8200.7677962939197}]
["Svovldioxid (SO2)",{"$f":"Emissioner_rute1_2_svovl-Emissioner_rute1_1_svovl","v":387.95741207057256},{"$f":"IF(Emissioner_rute1_2_svovl=0,\"Kan ikke udregnes\",(Emissioner_rute1_2_svovl-Emissioner_rute1_1_svovl)/Emissioner_rute1_2_svovl)","v":0.47687031860635332},"Svovldioxid (SO2)",{"$f":"Pris_rute1_2_svovl-Pris_rute1_1_svovl","v":80.986109769732025}]
["Kvælstofilter (NOx)",{"$f":"Emissioner_rute1_2_kvæl-Emissioner_rute1_1_kvæl","v":447989.45406238915},{"$f":"IF(Emissioner_rute1_2_kvæl=0,\"Kan ikke udregnes\",(Emissioner_rute1_2_kvæl-Emissioner_rute1_1_kvæl)/Emissioner_rute1_2_kvæl)","v":0.94398965472967045},"Kvælstofilter (NOx)",{"$f":"Pris_rute1_2_kvæl-Pris_rute1_1_kvæl","v":21503.49379499468}]
["Kulilte (CO)",{"$f":"Emissioner_rute1_2_kulilt-Emissioner_rute1_1_kulilt","v":99641.35225084766},{"$f":"IF(Emissioner_rute1_2_kulilt=0,\"Kan ikke udregnes\",(Emissioner_rute1_2_kulilt-Emissioner_rute1_1_kulilt)/Emissioner_rute1_2_kulilt)","v":0.49990763151491424},"Kulilte (CO)",{"$f":"Pris_rute1_2_kulilt-Pris_rute1_1_kulilt","v":1.6440823121389865}]
["Kulbrinte (HC) ",{"$f":"Emissioner_rute1_2_kulbrint-Emissioner_rute1_1_kulbrint","v":54004.504584318362},{"$f":"IF(Emissioner_rute1_2_kulbrint=0,\"Kan ikke udregnes\",(Emissioner_rute1_2_kulbrint-Emissioner_rute1_1_kulbrint)/Emissioner_rute1_2_kulbrint)","v":0.86209574081168849},"Kulbrinte (HC) ",{"$f":"Pris_rute1_2_kulbrint-Pris_rute1_1_kulbrint","v":148.51238760687548}]
["Partikler (PM)",{"$f":"Emissioner_rute1_2_part-Emissioner_rute1_1_part","v":9441.5669219394731},{"$f":"IF(Emissioner_rute1_2_part=0,\"Kan ikke udregnes\",(Emissioner_rute1_2_part-Emissioner_rute1_1_part)/Emissioner_rute1_2_part)","v":0.99474903013090654},"Partikler (PM)",{"$f":"Pris_rute1_2_part-Pris_rute1_1_part","v":11603.685747063613}]
[null,null,null,"Samlede årlige miljøbesparelse ved gennemførelse af tiltag på rute 1",{"$f":"SUM(Besparelse_rute1_kul:Besparelse_rute1_part)","v":41539.089918040961}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,{"$f":"IF(Brændstof_rute13_1=\"El\",\"Ikke oplyst\",IF(Okochau_rute13_1=\"Ja\",AntalKM_rute13/Forbrug_rute13_1*(1-Bbesparelse_rute13_1)*(1-OkoVærdi),AntalKM_rute13/Forbrug_rute13_1*(1-Bbesparelse_rute13_1)))","v":{"$error":"#REF!"}}]

{"sheet":"Ruteoplysninger","index":1,"n_rows":5,"n_cols":2,"rows_kept":5,"cut":false,"hidden":false,"merged":[[0,0,0,1]]}
["Ruteoplysninger"]
["Rute 1"]
["Antal rutekilometer årligt",120000]
["Andel bykørsel",0.75]
["Gennemsnitshastighed","34 km/t"]

{"sheet":"Brændstoftyper","index":2,"n_rows":81,"n_cols":17,"rows_kept":81,"cut":false,"hidden":false,"merged":[]}
["Euro-normer","Euro 6","EEV","Euro 5","Euro 4","Euro 3","Euro 2"]
["Kvælstofilter (NOx) (g/kWh)",0.4,2,2,3.5,5,7,null,null,"Emissioner i alternative drivmidler","Diesel","Biodiesel (100% RME)","Naturgas (CNG)","Biogas (BNG)","Ethanol (E100)","El","Brint"]
["Kulilte (CO) (g/kWh)",1.5,1.5,1.5,1.5,2.1,4,null,null,"Kuldioxid (CO2) (g/MJ)",74,0,57,0,0,0,0]
["Kulbrinte (HC) (g/kWh)",0.13,0.25,0.46,0.46,0.66,1.1000000000000001,null,null,"Svovldioxid (SO2) (g/MJ)",5.0000000000000001E-4,5.0000000000000001E-4,0,0,3.8999999999999999E-4,0,0]
["Partikler (PM) (g/kWh)",0.01,0.02,0.02,0.02,0.1,0.15,null,null,"Kvælstofilter (NOx) (g/MJ)",0.68289999999999995,0.68289999999999995,1.617E-2,1.6199999999999999E-2,1.7090000000000001E-2,0,0]
[null,null,null,null,null,null,null,null,null,"Kulilte (CO) (g/MJ)","IA",0,0,0,0,0,0]
["Euro-normer","Euro 6","EEV","Euro 5","Euro 4","Euro 3","Euro 2",null,null,"Kulbrinte (HC) (g/MJ)","IA",0,0,0,0,0,0]
["Kvælstofilter (NOx) (g/MJ)",{"$f":"B2/$B$81","v":0.11111111111111112},0.55555555555555558,0.55555555555555558,0.97222222222222221,1.3888888888888888,1.9444444444444444,null,null,"Partikler (PM) (g/MJ)","IA",9.41E-3,0,0,0,0,0]
["Kulilte (CO) (g/MJ)",0.41666666666666663,0.41666666666666663,0.41666666666666663,0.41666666666666663,0.58333333333333337,1.1111111111111112]
["Kulbrinte (HC) (g/MJ)",3.6111111111111115E-2,6.9444444444444448E-2,0.12777777777777777,0.12777777777777777,0.18333333333333335,0.30555555555555558]
["Partikler (PM) (g/MJ)",2.7777777777777779E-3,5.5555555555555558E-3,5.5555555555555558E-3,5.5555555555555558E-3,2.777777777777778E-2,4.1666666666666664E-2]
[]
[null,"Diesel","Biodiesel (100% RME)","Naturgas (CNG)","Biogas (BNG)","Ethanol (E100)","El","Brint"]
["Brændselsværdier i motor (MJ/l el. MJ/Nm3)",35.5,{"$f":"35.5*(1-0.126)","v":31.027000000000001},39.6,39.6,21.4]
["kWh i brændstof",{"$f":"B14*$B80","v":9.8583499999999997},{"$f":"C14*$B80","v":8.6161978999999995},{"$f":"D14*$B80","v":10.996920000000001},{"$f":"E14*$B80","v":10.996920000000001},{"$f":"F14*$B80","v":5.94278}]
["Motorens virkningsgrad",0.21,0.21,0.16,0.16,0.16,0.79]
["Energiudnyttelse (MJ/l)",{"$f":"B16*B14","v":7.4550000000000001},{"$f":"C16*C14","v":6.5156700000000001},{"$f":"D16*D14","v":6.3360000000000003},{"$f":"E16*E14","v":6.3360000000000003},{"$f":"F16*F14","v":3.4239999999999999}]
["Udnyttet kWh i brændstof (kWh/l el. kWh/Nm3)",{"$f":"B17*$B80","v":2.0702535000000002},{"$f":"C17*$B80","v":1.8094015590000001},{"$f":"D17*$B80","v":1.7595072},{"$f":"E17*$B80","v":1.7595072},{"$f":"F17*$B80","v":0.95084479999999993}]
[]
[]
["Effektive emissioner i g/l el. g/Nm3"]
["Euro 6","Diesel","Biodiesel (100% RME)","Naturgas (CNG)","Biogas (BNG)","Ethanol (E100)","El","Brint"]
["Kuldioxid (CO2) (g/l)",{"$f":"B$14*K3","v":2627},{"$f":"C$14*L3","v":0},{"$f":"D$14*M3","v":2257.2000000000003},{"$f":"E$14*N3","v":0},{"$f":"F$14*O3","v":0},{"$f":"G$17*P3","v":0},0]
["Svovldioxid (SO2) (g/l)",{"$f":"B$14*K4","v":1.7750000000000002E-2},{"$f":"C17*L4","v":3.2578350000000002E-3},{"$f":"D$14*M4","v":0},0,8.3459999999999993E-3,0,0]
["Kvælstofilter (NOx) (g/l)",{"$f":"$B$8*B$17","v":0.82833333333333337},{"$f":"$B8*C$17","v":0.7239633333333334},0.64033200000000001,0.64151999999999998,0.365726,0,0]
["Kulilte (CO) (g/l)",{"$f":"B9*B$17","v":3.1062499999999997},{"$f":"$B9*C$17","v":2.7148624999999997},0,0,0,0,0]
["Kulbrinte (HC) (g/l)",{"$f":"B10*B$17","v":0.26920833333333338},{"$f":"$B10*C$17","v":0.23528808333333337},0,0,0,0,0]
["Partikler (PM) (g/l)",{"$f":"B11*B$17","v":2.0708333333333336E-2},{"$f":"$B11*C$17","v":1.8099083333333335E-2},0,0,0,0,0]
[]
["Effektive emissioner i g/l el. g/Nm3"]
["EEV","Diesel","Biodiesel (100% RME)","Naturgas (CNG)","Biogas (BNG)","Ethanol (E100)","El","Brint"]
["Kuldioxid (CO2) (g/l)",{"$f":"B23","v":2627},0,2257.2000000000003,0,0,0,0]
["Svovldioxid (SO2) (g/l)",1.7750000000000002E-2,3.2578350000000002E-3,0,0,8.3459999999999993E-3,0,0]
["Kvælstofilter (NOx) (g/l)",{"$f":"$C$8*B$17","v":4.1416666666666666},{"$f":"$C8*C$17","v":3.6198166666666669},{"$f":"D25","v":0.64033200000000001},0.64151999999999998,0.365726,0,0]
["Kulilte (CO) (g/l)",{"$f":"C9*$B$17","v":3.1062499999999997},{"$f":"$C9*C$17","v":2.7148624999999997},0,0,0,0,0]
["Kulbrinte (HC) (g/l)",{"$f":"C10*$B$17","v":0.51770833333333333},{"$f":"$C10*C$17","v":0.45247708333333336},0,0,0,0,0]
["Partikler (PM) (g/l)",{"$f":"C11*$B$17","v":4.1416666666666671E-2},{"$f":"$C11*C$17","v":3.619816666666667E-2},0,0,0,0,0]
[]
["Effektive emissioner i g/l el. g/Nm3"]
["Euro 5","Diesel","Biodiesel (100% RME)","Naturgas (CNG)","Biogas (BNG)","Ethanol (E100)","El","Brint"]
["Kuldioxid (CO2) (g/l)",{"$f":"B32","v":2627},0,2257.2000000000003,0,0,0,0]
["Svovldioxid (SO2) (g/l)",{"$f":"B33","v":1.7750000000000002E-2},{"$f":"C33","v":3.2578350000000002E-3},{"$f":"D33","v":0},0,8.3459999999999993E-3,0,0]
["Kvælstofilter (NOx) (g/l)",{"$f":"$D8*B$17","v":4.1416666666666666},{"$f":"$D8*C$17","v":3.6198166666666669},0.64033200000000001,0.64151999999999998,0.365726,0,0]
["Kulilte (CO) (g/l)",{"$f":"D9*$B$17","v":3.1062499999999997},{"$f":"$D9*C$17","v":2.7148624999999997},0,0,0,0,0]
["Kulbrinte (HC) (g/l)",{"$f":"D10*$B$17","v":0.95258333333333323},{"$f":"$D10*C$17","v":0.83255783333333333},0,0,0,0,0]
["Partikler (PM) (g/l)",{"$f":"D11*$B$17","v":4.1416666666666671E-2},{"$f":"$D11*C$17","v":3.619816666666667E-2},0,0,0,0,0]
[]
["Effektive emissioner i g/l el. g/Nm3"]
["Euro 4","Diesel","Biodiesel (100% RME)","Naturgas (CNG)","Biogas (BNG)","Ethanol (E100)","El","Brint"]
["Kuldioxid (CO2) (g/l)",{"$f":"B41","v":2627},0,2257.2000000000003,0,0,0,0]
["Svovldioxid (SO2) (g/l)",{"$f":"B42","v":1.7750000000000002E-2},{"$f":"C42","v":3.2578350000000002E-3},{"$f":"D42","v":0},0,8.3459999999999993E-3,0,0]
["Kvælstofilter (NOx) (g/l)",{"$f":"$E8*B$17","v":7.2479166666666668},{"$f":"$E8*C$17","v":6.3346791666666666},0.64033200000000001,0.64151999999999998,0.365726,0,0]
["Kulilte (CO) (g/l)",{"$f":"E9*$B$17","v":3.1062499999999997},{"$f":"$E9*C$17","v":2.7148624999999997},0,0,0,0,0]
["Kulbrinte (HC) (g/l)",{"$f":"E10*$B$17","v":0.95258333333333323},{"$f":"$E10*C$17","v":0.83255783333333333},0,0,0,0,0]
["Partikler (PM) (g/l)",{"$f":"E11*$B$17","v":4.1416666666666671E-2},{"$f":"$E11*C$17","v":3.619816666666667E-2},0,0,0,0,0]
[]
["Effektive emissioner i g/l el. g/Nm3"]
["Euro 3","Diesel","Biodiesel (100% RME)","Naturgas (CNG)","Biogas (BNG)","Ethanol (E100)","El","Brint"]
["Kuldioxid (CO2) (g/l)",{"$f":"B50","v":2627},0,2257.2000000000003,0,0,0,0]
["Svovldioxid (SO2) (g/l)",{"$f":"B51","v":1.7750000000000002E-2},{"$f":"C51","v":3.2578350000000002E-3},{"$f":"D51","v":0},0,8.3459999999999993E-3,0,0]
["Kvælstofilter (NOx) (g/l)",{"$f":"$F8*B$17","v":10.354166666666666},{"$f":"$F8*C$17","v":9.0495416666666664},0.64033200000000001,0.64151999999999998,0.365726,0,0]
["Kulilte (CO) (g/l)",{"$f":"F9*$B$17","v":4.3487499999999999},{"$f":"$F9*C$17","v":3.8008075000000003},0,0,0,0,0]
["Kulbrinte (HC) (g/l)",{"$f":"F10*$B$17","v":1.3667500000000001},{"$f":"$F10*C$17","v":1.1945395000000001},0,0,0,0,0]
["Partikler (PM) (g/l)",{"$f":"F11*$B$17","v":0.20708333333333334},{"$f":"$F11*C$17","v":0.18099083333333335},0,0,0,0,0]
[]
["Effektive emissioner i g/l el. g/Nm3"]
["Euro 2","Diesel","Biodiesel (100% RME)","Naturgas (CNG)","Biogas (BNG)","Ethanol (E100)","El","Brint"]
["Kuldioxid (CO2) (g/l)",{"$f":"B59","v":2627},0,2257.2000000000003,0,0,0,0]
["Svovldioxid (SO2) (g/l)",{"$f":"B60","v":1.7750000000000002E-2},{"$f":"C60","v":3.2578350000000002E-3},{"$f":"D60","v":0},0,8.3459999999999993E-3,0,0]
["Kvælstofilter (NOx) (g/l)",{"$f":"$G8*B$17","v":14.495833333333334},{"$f":"$G8*C$17","v":12.669358333333333},0.64033200000000001,0.64151999999999998,0.365726,0,0]
["Kulilte (CO) (g/l)",{"$f":"$G9*B$17","v":8.2833333333333332},7.2396333333333338,0,0,0,0,0]
["Kulbrinte (HC) (g/l)",2.277916666666667,1.9908991666666669,0,0,0,0,0]
["Partikler (PM) (g/l)",0.31062499999999998,0.27148624999999998,0,0,0,0,0]
[]
[]
[]
[]
[{"$f":"'Andre tiltag'!A2","v":"Partikelfilter"},{"$f":"'Andre tiltag'!C2","v":0.92500000000000004}]
[{"$f":"'Andre tiltag'!A3","v":"Økochauffør "},{"$f":"'Andre tiltag'!C3","v":0.11}]
[{"$f":"'Andre tiltag'!A4","v":"MJ til KWH"},{"$f":"'Andre tiltag'!C4","v":0.2777}]
["kWh til MJ",{"$f":"'Andre tiltag'!C5","v":3.6}]

{"sheet":"Emissionspriser","index":3,"n_rows":21,"n_cols":7,"rows_kept":21,"cut":false,"hidden":false,"merged":[[15,0,15,2]]}
[null,"Kuldioxid (CO2)","Svovldioxid (SO2)","Kvælstofilter (NOx)","Kulilte (CO)","Kulbrinte (HC)","Partikler (PM2,5)"]
["Emisssionspriser Land"]
["Lavt estimat",0.08,10,0,0,0,31]
["Middel estimat",0.13,187,48,8.0000000000000002E-3,2,218]
["Højt estimat",0.25,1128,336,0.99299999999999999,13,1475]
["Emissionspriser By"]
["Lavt estimat",0.08,51,4,4.0000000000000001E-3,1,224]
["Middel estimat",0.13,216,48,2.1999999999999999E-2,3,1566]
["Højt estimat",0.25,1027,366,2.7749999999999999,15,10577]
["Vægtning af enkelte udledninger",1,1,1,1,1,1]
[]
["Generelle estimationsforudsætninger","Middel estimat"]
[]
[]
[]
["Note: Priser for udledninger af partikler og gas er opgjort i kr./kg.\nPriser for støj er opgjort i kr./SBT"]
[]
[]
[null,"Kuldioxid (CO2)","Partikler (PM2,5)","Kvælstofilter (NOx)","Kulilte (CO)","Kulbrinte (HC)","Svovldioxid (SO2)"]
["Emisssionspriser Land givet estimat ",{"$f":"IF(ValgEstimat=\"Lavt estimat\",B3,IF(ValgEstimat=\"Middel estimat\",B4,IF(ValgEstimat=\"Højt estimat\",B5,\"fejl\")))","v":0.13},{"$f":"IF(ValgEstimat=\"Lavt estimat\",G3,IF(ValgEstimat=\"Middel estimat\",G4,IF(ValgEstimat=\"Højt estimat\",G5,\"fejl\")))","v":218},{"$f":"IF(ValgEstimat=\"Lavt estimat\",D3,IF(ValgEstimat=\"Middel estimat\",D4,IF(ValgEstimat=\"Højt estimat\",D5,\"fejl\")))","v":48},{"$f":"IF(ValgEstimat=\"Lavt estimat\",E3,IF(ValgEstimat=\"Middel estimat\",E4,IF(ValgEstimat=\"Højt estimat\",E5,\"fejl\")))","v":8.0000000000000002E-3},{"$f":"IF(ValgEstimat=\"Lavt estimat\",F3,IF(ValgEstimat=\"Middel estimat\",F4,IF(ValgEstimat=\"Højt estimat\",F5,\"fejl\")))","v":2},{"$f":"IF(ValgEstimat=\"Lavt estimat\",C3,IF(ValgEstimat=\"Middel estimat\",C4,IF(ValgEstimat=\"Højt estimat\",C5,\"fejl\")))","v":187}]
["Emissionspriser By givet estimat",{"$f":"IF(ValgEstimat=\"Lavt estimat\",B7,IF(ValgEstimat=\"Middel estimat\",B8,IF(ValgEstimat=\"Højt estimat\",B9,\"fejl\")))","v":0.13},{"$f":"IF(ValgEstimat=\"Lavt estimat\",G7,IF(ValgEstimat=\"Middel estimat\",G8,IF(ValgEstimat=\"Højt estimat\",G9,\"fejl\")))","v":1566},{"$f":"IF(ValgEstimat=\"Lavt estimat\",D7,IF(ValgEstimat=\"Middel estimat\",D8,IF(ValgEstimat=\"Højt estimat\",D9,\"fejl\")))","v":48},{"$f":"IF(ValgEstimat=\"Lavt estimat\",E7,IF(ValgEstimat=\"Middel estimat\",E8,IF(ValgEstimat=\"Højt estimat\",E9,\"fejl\")))","v":2.1999999999999999E-2},{"$f":"IF(ValgEstimat=\"Lavt estimat\",F7,IF(ValgEstimat=\"Middel estimat\",F8,IF(ValgEstimat=\"Højt estimat\",F9,\"fejl\")))","v":3},{"$f":"IF(ValgEstimat=\"Lavt estimat\",C7,IF(ValgEstimat=\"Middel estimat\",C8,IF(ValgEstimat=\"Højt estimat\",C9,\"fejl\")))","v":216}]

{"sheet":"Andre tiltag","index":4,"n_rows":5,"n_cols":6,"rows_kept":5,"cut":false,"hidden":false,"merged":[]}
[null,"Effekt",null,null,null,"PF-værdi"]
["Partikelfilter","Det antages at partikelfiltre tilbageholder:",0.92500000000000004,"af partikelemissionen",null,{"$f":"1-Partikelfiltereffekt","v":7.4999999999999956E-2}]
["Økochauffør ","Det antages at økochaufførkurser mindsker brændstoffobruget med:",0.11]
["MJ til KWH","Omregningsfaktor",0.2777]
["kWh til MJ","Omregningsfaktor",3.6]

{"sheet":"Brændstofforbrug","index":5,"n_rows":342,"n_cols":163,"rows_kept":342,"cut":false,"hidden":true,"merged":[[2,29,2,30],[2,15,2,16],[2,17,2,18],[2,21,2,22],[2,23,2,24],[2,27,2,28],[2,59,2,60],[2,111,2,112],[2,113,2,114],[2,123,2,124],[2,125,2,126],[2,75,2,76],[2,77,2,78],[2,87,2,88],[2,89,2,90],[2,99,2,100],[2,101,2,102],[2,63,2,64],[2,65,2,66],[2,95,2,96],[2,69,2,70],[2,71,2,72],[2,33,2,34],[2,35,2,36],[2,45,2,46],[2,47,2,48],[2,57,2,58],[2,39,2,40],[2,41,2,42],[2,51,2,52],[2,53,2,54],[2,147,2,148],[2,149,2,150],[2,159,2,160],[2,161,2,162],[2,135,2,136],[2,137,2,138],[2,153,2,154],[2,155,2,156],[2,81,2,82],[2,83,2,84],[2,93,2,94],[2,141,2,142],[2,143,2,144],[2,105,2,106],[2,107,2,108],[2,117,2,118],[2,119,2,120],[2,129,2,130],[2,131,2,132]]}
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Reelt brændstofforbrug rute 1",null,"Tiltag",null,"Sammenligning",null,"Reelt brændstofforbrug rute 2",null,"Tiltag",null,"Sammenligning",null,"Reelt brændstofforbrug rute 3",null,"Tiltag",null,"Sammenligning",null,"Reelt brændstofforbrug rute 4",null,"Tiltag",null,"Sammenligning",null,"Reelt brændstofforbrug rute 5",null,"Tiltag",null,"Sammenligning",null,"Reelt brændstofforbrug rute 6",null,"Tiltag",null,"Sammenligning",null,"Reelt brændstofforbrug rute 7",null,"Tiltag",null,"Sammenligning",null,"Reelt brændstofforbrug rute 8",null,"Tiltag",null,"Sammenligning",null,"Reelt brændstofforbrug rute 9",null,"Tiltag",null,"Sammenligning",null,"Reelt brændstofforbrug rute 10",null,"Tiltag",null,"Sammenligning",null,"Reelt brændstofforbrug rute 11",null,"Tiltag",null,"Sammenligning",null,"Reelt brændstofforbrug rute 12",null,"Tiltag",null,"Sammenligning",null,"Reelt brændstofforbrug rute 13",null,"Tiltag",null,"Sammenligning",null,"Reelt brændstofforbrug rute 14",null,"Tiltag",null,"Sammenligning",null,"Reelt brændstofforbrug rute 15",null,"Tiltag",null,"Sammenligning",null,"Reelt brændstofforbrug rute 16",null,"Tiltag",null,"Sammenligning",null,"Reelt brændstofforbrug rute 17",null,"Tiltag",null,"Sammenligning",null,"Reelt brændstofforbrug rute 18",null,"Tiltag",null,"Sammenligning",null,"Reelt brændstofforbrug rute 19",null,"Tiltag",null,"Sammenligning",null,"Reelt brændstofforbrug rute 20",null,"Tiltag",null,"Sammenligning",null,"Reelt brændstofforbrug rute 21",null,"Tiltag",null,"Sammenligning",null,"Reelt brændstofforbrug rute 22",null,"Tiltag",null,"Sammenligning",null,"Reelt brændstofforbrug rute 23",null,"Tiltag",null,"Sammenligning",null,"Reelt brændstofforbrug rute 24",null,"Tiltag",null,"Sammenligning",null,"Reelt brændstofforbrug rute 25",null,"Tiltag",null,"Sammenligning"]
["Busstørrelse","Hastighed km/t","Euro 6","EEV","Euro 5","Euro 4","Euro 3","Euro 2","Biodiesel","Ethanol","Gas",null,null,"Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol"]
["10 meter",10,2.843776898898601,2.7609484455326223,2.9303775071915283,2.6534055529699532,2.3795315245209538,2.5359699420592392,2.7299702063721822,1.7677528252066277,2.9069715535001404,null,null,"10 meter",10,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_10*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_10*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.8039445565143546},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_10*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_10*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.4671684731064105},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_10*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_10*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.843776898898601},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_10*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_10*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.843776898898601},"10 meter",10,null,null,null,null,"10 meter",10,null,null,null,null,"10 meter",10,null,null,null,null,"10 meter",10,null,null,null,null,"10 meter",10,null,null,null,null,"10 meter",10,null,null,null,null,"10 meter",10,null,null,null,null,"10 meter",10,null,null,null,null,"10 meter",10,null,null,null,null,"10 meter",10,null,null,null,null,"10 meter",10,null,null,null,null,"10 meter",10,null,null,null,null,"10 meter",10,null,null,null,null,"10 meter",10,null,null,null,null,"10 meter",10,null,null,null,null,"10 meter",10,null,null,null,null,"10 meter",10,null,null,null,null,"10 meter",10,null,null,null,null,"10 meter",10,null,null,null,null,"10 meter",10,null,null,null,null,"10 meter",10,null,null,null,null,"10 meter",10,null,null,null,null,"10 meter",10,null,null,null,null,"10 meter",10]
[null,11,2.8837624843129266,2.7997694022455599,2.9584077193828171,2.6839973790496887,2.4088643695156167,2.559631394548294,2.768056005653698,1.7926087242791222,2.9478457020293423,null,null,null,11,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_11*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_11*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.8432652167821963},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_11*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_11*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.5018586683010948},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_11*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_11*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.8837624843129266},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_11*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_11*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.8837624843129266},null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11]
[null,12,2.9237480697272522,2.8385903589584971,2.9864379315741059,2.7145892051294243,2.4381972145102799,2.5832928470373484,2.8061339185843264,1.8174646233516167,2.9887198505585442,null,null,null,12,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_12*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_12*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.8825831168272282},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_12*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_12*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.5365488634957796},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_12*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_12*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.9237480697272522},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_12*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_12*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.9237480697272522},null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12]
[null,13,2.9637336551415769,2.8774113156714343,3.0144681437653951,2.7451810312091598,2.4675300595049432,2.6069542995264023,2.8442039615681511,1.8423205224241106,3.0295939990877452,null,null,null,13,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_13*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_13*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.921898262390878},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_13*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_13*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.5712390586904639},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_13*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_13*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.9637336551415769},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_13*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_13*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.9637336551415769},null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13]
[null,14,3.0037192405559026,2.9162322723843714,3.0424983559566838,2.7757728572888949,2.496862904499606,2.6306157520154567,2.8822661509637917,1.8671764214966051,3.0704681476169471,null,null,null,14,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_14*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_14*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.961210659198664},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_14*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_14*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.6059292538851486},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_14*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_14*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.0037192405559026},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_14*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_14*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.0037192405559026},null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14]
[null,15,3.0437048259702286,2.9550532290973091,3.0705285681479726,2.8063646833686304,2.5261957494942693,2.6542772045045115,2.9203205030845609,1.8920323205690999,3.1113422961461494,null,null,null,15,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_15*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_15*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.0005203129602451},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_15*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_15*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.6406194490798338},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_15*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_15*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.0437048259702286},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_15*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_15*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.0437048259702286},null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15]
[null,16,3.0836904113845534,2.9938741858102462,3.0985587803392618,2.836956509448366,2.5555285944889325,2.6779386569935655,2.9583670341986208,1.9168882196415939,3.1522164446753504,null,null,null,16,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_16*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_16*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.039827229369477},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_16*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_16*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.6753096442745177},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_16*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_16*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.0836904113845534},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_16*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_16*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.0836904113845534},null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16]
[null,17,3.123675996798879,3.0326951425231834,3.1265889925305506,2.8675483355281011,2.5848614394835954,2.7016001094826199,2.9964057605291416,1.9417441187140885,3.1930905932045528,null,null,null,17,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_17*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_17*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.079131414104471},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_17*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_17*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.7099998394692024},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_17*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_17*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.123675996798879},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_17*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_17*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.123675996798879},null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17]
[null,18,3.1636615822132046,3.0715160992361206,3.1546192047218393,2.8981401616078366,2.6141942844782586,2.7252615619716747,3.0344366982544542,1.966600017786583,3.2339647417337547,null,null,null,18,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_18*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_18*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.1184328728276416},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_18*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_18*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.7446900346638872},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_18*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_18*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1636615822132046},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_18*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_18*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1636615822132046},null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18]
[null,19,3.2036471676275293,3.1103370559490631,3.1826494169131281,2.9287319876875721,2.6435271294729219,2.7489230144607286,3.072459863508207,1.9914559168590769,3.2748388902629557,null,null,null,19,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_19*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_19*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.1577316111857665},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_19*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_19*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.779380229858571},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_19*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_19*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.2036471676275293},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_19*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_19*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.2036471676275293},null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19]
[null,20,3.2436327530418554,3.1491580126619954,3.2106796291044173,2.9593238137673072,2.6728599744675847,2.772584466949783,3.1104752723795195,2.0163118159315716,3.3157130387921581,null,null,null,20,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_20*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_20*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.1970276348100377},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_20*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_20*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.8140704250532562},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_20*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_20*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.2436327530418554},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_20*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_20*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.2436327530418554},null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20]
[null,21,3.2836183384561806,3.1879789693749325,3.2387098412957065,2.9899156398470432,2.702192819462248,2.7962459194388378,3.1484829409131336,2.0411677150040659,3.3565871873213595,null,null,null,21,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_21*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_21*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.2363209493161138},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_21*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_21*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.8487606202479405},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_21*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_21*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.2836183384561806},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_21*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_21*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.2836183384561806},null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21]
[null,22,3.3236039238705057,3.2267999260878697,3.2667400534869948,3.0205074659267783,2.7315256644569113,2.8199073719278922,3.1864828851095703,2.0660236140765602,3.397461335850561,null,null,null,22,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_22*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_22*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.2756115603041787},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_22*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_22*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.8834508154426248},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_22*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_22*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.3236039238705057},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_22*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_22*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.3236039238705057},null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22]
[null,23,3.3635895092848318,3.2656208828008073,3.294770265678284,3.0510992920065139,2.7608585094515745,2.8435688244169461,3.2244751209252809,2.090879513149055,3.4383354843797633,null,null,null,23,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_23*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_23*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.3148994733589889},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_23*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_23*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.91814101063731},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_23*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_23*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.3635895092848318},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_23*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_23*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.3635895092848318},null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23]
[null,24,3.4035750946991565,3.304441839513744,3.3228004778695723,3.081691118086249,2.7901913544462373,2.867230276906001,3.2624596642727948,2.1157354122215488,3.4792096329089643,null,null,null,24,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_24*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_24*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.3541846940499296},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_24*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_24*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.9528312058319939},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_24*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_24*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.4035750946991565},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_24*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_24*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.4035750946991565},null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24]
[null,25,3.4435606801134822,3.3432627962266817,3.3508306900608615,3.1122829441659845,2.8195241994409006,2.8908917293950553,3.3004365310208765,2.1405913112940436,3.5200837814381662,null,null,null,25,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_25*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_25*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.3934672279310698},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_25*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_25*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.9875214010266786},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_25*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_25*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.4435606801134822},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_25*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_25*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.4435606801134822},null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25]
[null,26,3.4835462655278073,3.3820837529396188,3.3788609022521503,3.14287477024572,2.8488570444355634,2.9145531818841097,3.3384057369946709,2.1654472103665374,3.5609579299673677,null,null,null,26,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_26*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_26*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.4327470805412097},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_26*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_26*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.0222115962213629},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_26*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_26*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.4835462655278073},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_26*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_26*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.4835462655278073},null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26]
[null,27,3.5235318509421329,3.420904709652556,3.4068911144434395,3.1734665963254551,2.8781898894302267,2.9382146343731637,3.3763672979758574,2.1903031094390322,3.6018320784965696,null,null,null,27,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_27*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_27*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.4720242574039366},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_27*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_27*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.0569017914160477},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_27*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_27*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.5235318509421329},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_27*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_27*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.5235318509421329},null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27]
[null,28,3.563517436356459,3.4597256663654941,3.4349213266347278,3.2040584224051911,2.9075227344248904,2.9618760868622185,3.4143212297027943,2.2151590085115269,3.642706227025772,null,null,null,28,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_28*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_28*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.5112987640276767},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_28*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_28*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.0915919866107329},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_28*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_28*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.563517436356459},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_28*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_28*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.563517436356459},null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28]
[null,29,3.6035030217707837,3.4985466230784312,3.462951538826017,3.2346502484849262,2.9368555794195537,2.9855375393512729,3.4522675478706715,2.2400149075840208,3.683580375554973,null,null,null,29,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_29*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_29*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.5505706059057447},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_29*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_29*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.1262821818054167},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_29*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_29*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.6035030217707837},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_29*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_29*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.6035030217707837},null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29]
[null,30,3.6434886071851094,3.5373675797913684,3.4909817510173053,3.2652420745646618,2.9661884244142165,3.0091989918403268,3.4902062681316557,2.2648708066565155,3.7244545240841749,null,null,null,30,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_30*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_30*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.5898397885164011},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_30*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_30*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.1609723770001015},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_30*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_30*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.6434886071851094},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_30*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_30*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.6434886071851094},null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30]
[null,31,3.6834741925994354,3.576188536504306,3.5190119632085946,3.2958339006443969,2.9955212694088797,3.0328604443293816,3.5281374060950412,2.2897267057290103,3.7653286726133777,null,null,null,31,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_31*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_31*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.629106317322897},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_31*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_31*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.1956625721947862},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_31*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_31*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.6834741925994354},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_31*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_31*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.6834741925994354},null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31]
[null,32,3.7234597780137597,3.6150094932172427,3.5470421753998838,3.3264257267241328,3.0248541144035426,3.056521896818436,3.5660609773273895,2.3145826048015037,3.8062028211425782,null,null,null,32,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_32*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_32*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.6683701977735304},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_32*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_32*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.2303527673894701},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_32*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_32*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.7234597780137597},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_32*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_32*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.7234597780137597},null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32]
[null,33,3.7634453634280858,3.6538304499301804,3.5750723875911725,3.3570175528038679,3.0541869593982058,3.0801833493074899,3.6039769973526852,2.3394385038739984,3.8470769696717806,null,null,null,33,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_33*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_33*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.7076314353016953},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_33*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_33*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.2650429625841553},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_33*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_33*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.7634453634280858},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_33*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_33*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.7634453634280858},null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33]
[null,34,3.8034309488424105,3.6926514066431175,3.6031025997824617,3.387609378883603,3.0835198043928691,3.1038448017965448,3.6418854816524728,2.3642944029464927,3.8879511182009816,null,null,null,34,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_34*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_34*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.746890035325932},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_34*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_34*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.2997331577788391},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_34*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_34*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.8034309488424105},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_34*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_34*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.8034309488424105},null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34]
[null,35,3.8434165342567361,3.7314723633560547,3.63113281197375,3.418201204963339,3.1128526493875324,3.1275062542855991,3.6797864456660072,2.389150302018987,3.9288252667301835,null,null,null,35,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_35*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_35*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.7861460032499812},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_35*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_35*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.3344233529735239},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_35*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_35*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.8434165342567361},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_35*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_35*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.8434165342567361},null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35]
[null,36,3.8834021196710622,3.7702933200689923,3.6591630241650392,3.4487930310430741,3.1421854943821952,3.1511677067746531,3.7176799047903955,2.4140062010914818,3.9696994152593859,null,null,null,36,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_36*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_36*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.8253993444628289},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_36*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_36*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.3691135481682091},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_36*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_36*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.8834021196710622},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_36*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_36*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.8834021196710622},null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36]
[null,37,3.9233877050853865,3.809114276781929,3.6871932363563276,3.4793848571228096,3.1715183393768585,3.1748291592637079,3.7555658743807396,2.4388621001639756,4.0105735637885864,null,null,null,37,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_37*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_37*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.8646500643387602},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_37*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_37*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.4038037433628929},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_37*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_37*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.9233877050853865},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_37*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_37*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.9233877050853865},null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37]
[null,38,3.9633732904997125,3.8479352334948667,3.7152234485476168,3.5099766832025447,3.2008511843715213,3.1984906117527623,3.7934443697502838,2.4637179992364704,4.0514477123177883,null,null,null,38,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_38*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_38*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.9038981682374123},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_38*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_38*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.4384939385575777},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_38*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_38*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.9633732904997125},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_38*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_38*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.9633732904997125},null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38]
[null,39,4.0033588759140377,3.8867561902078038,3.743253660738906,3.5405685092822807,3.2301840293661845,3.2221520642418167,3.8313154061705523,2.4885738983089647,4.0923218608469902,null,null,null,39,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_39*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_39*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.943143661503818},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_39*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_39*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.473184133752262},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_39*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_39*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.0033588759140377},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_39*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_39*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.0033588759140377},null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39]
[null,40,4.0433444613283633,3.925577146920741,3.7712838729301947,3.5711603353620158,3.2595168743608478,3.2458135167308715,3.8691789988714933,2.513429797381459,4.1331960093761921,null,null,null,40,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_40*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_40*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.9823865494684587},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_40*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_40*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.5078743289469467},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_40*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_40*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.0433444613283633},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_40*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_40*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.0433444613283633},null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40]
[null,41,4.083330046742689,3.9643981036336786,3.7993140851214835,3.6017521614417518,3.2888497193555111,3.2694749692199254,3.9070351630416233,2.5382856964539533,4.174070157905394,null,null,null,41,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_41*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_41*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.0216268374473163},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_41*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_41*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.5425645241416319},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_41*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_41*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.083330046742689},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_41*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_41*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.083330046742689},null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41]
[null,42,4.1233156321570137,4.0032190603466162,3.8273442973127723,3.6323439875214869,3.3181825643501739,3.2931364217089798,3.9448839138281615,2.5631415955264476,4.2149443064345951,null,null,null,42,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_42*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_42*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.0608645307419149},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_42*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_42*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.5772547193363153},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_42*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_42*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.1233156321570137},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_42*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_42*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.1233156321570137},null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42]
[null,43,4.1633012175713393,4.042040017059553,3.855374509504061,3.662935813601222,3.3475154093448372,3.3167978741980346,3.9827252663371753,2.5879974945989419,4.255818454963797,null,null,null,43,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_43*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_43*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.1000996346393812},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_43*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_43*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.6119449145310001},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_43*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_43*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.1633012175713393},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_43*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_43*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.1633012175713393},null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43]
[null,44,4.2032868029856658,4.0808609737724906,3.8834047216953502,3.6935276396809575,3.3768482543395,3.3404593266870886,4.0205592356337192,2.6128533936714371,4.2966926034929998,null,null,null,44,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_44*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_44*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.1393321544124841},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_44*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_44*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.6466351097256857},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_44*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_44*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.2032868029856658},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_44*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_44*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.2032868029856658},null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44]
[null,45,4.2432723883999897,4.1196819304854273,3.911434933886639,3.7241194657606926,3.4061810993341632,3.3641207791761429,4.0583858367419703,2.6377092927439305,4.3375667520221999,null,null,null,45,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_45*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_45*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.1785620953196823},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_45*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_45*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.6813253049203687},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_45*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_45*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.2432723883999897},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_45*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_45*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.2432723883999897},null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45]
[null,46,4.2832579738143162,4.1585028871983649,3.9394651460779282,3.7547112918404286,3.4355139443288265,3.3877822316651978,4.0962050846453719,2.6625651918164257,4.3784409005514027,null,null,null,46,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_46*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_46*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.2177894626051859},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_46*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_46*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.7160155001150548},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_46*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_46*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.2832579738143162},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_46*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_46*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.2832579738143162},null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46]
[null,47,4.3232435592286409,4.1973238439113025,3.967495358269217,3.7853031179201642,3.4648467893234898,3.4114436841542517,4.1340169942867684,2.6874210908889196,4.4193150490806037,null,null,null,47,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_47*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_47*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.2570142614989859},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_47*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_47*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.7507056953097386},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_47*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_47*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.3232435592286409},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_47*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_47*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.3232435592286409},null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47]
[null,48,4.3632291446429665,4.2361448006242393,3.9955255704605057,3.8158949439998997,3.4941796343181526,3.4351051366433061,4.1718215805685439,2.7122769899614139,4.4601891976098056,null,null,null,48,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_48*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_48*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.2962364972169187},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_48*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_48*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.7853958905044234},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_48*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_48*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.3632291446429665},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_48*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_48*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.3632291446429665},null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48]
[null,49,4.4032147300572921,4.2749657573371769,4.023555782651794,3.8464867700796348,3.5235124793128159,3.4587665891323605,4.2096188583527567,2.7371328890339086,4.5010633461390075,null,null,null,49,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_49*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_49*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.3354561749607043},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_49*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_49*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.8200860856991081},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_49*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_49*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.4032147300572921},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_49*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_49*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.4032147300572921},null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49]
[null,50,4.4432003154716169,4.3137867140501136,4.0515859948430828,3.8770785961593699,3.5528453243074787,3.4824280416214148,4.2474088424612786,2.7619887881064025,4.5419374946682085,null,null,null,50,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_50*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_50*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.3746732999179985},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_50*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_50*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.854776280893792},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_50*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_50*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.4432003154716169},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_50*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_50*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.4432003154716169},null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50]
[null,51,4.4831859008859434,4.3526076707630512,4.0796162070343724,3.9076704222391054,3.5821781693021419,3.5060894941104697,4.2851915476759315,2.7868446871788977,4.5828116431974113,null,null,null,51,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_51*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_51*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.4138878772624395},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_51*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_51*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.8894664760884776},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_51*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_51*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.4831859008859434},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_51*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_51*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.4831859008859434},null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51]
[null,52,4.5231714863002681,4.3914286274759888,4.1076464192256612,3.938262248318841,3.6115110142968052,3.5297509465995236,4.3229669887386155,2.8117005862513915,4.6236857917266123,null,null,null,52,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_52*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_52*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.4530999121536894},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_52*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_52*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.9241566712831615},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_52*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_52*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.5231714863002681},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_52*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_52*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.5231714863002681},null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52]
[null,53,4.5631570717145937,4.4302495841889256,4.13567663141695,3.9688540743985765,3.6408438592914685,3.553412399088578,4.3607351803514556,2.8365564853238858,4.6645599402558142,null,null,null,53,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_53*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_53*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.4923094097374952},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_53*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_53*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.9588468664778462},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_53*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_53*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.5631570717145937},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_53*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_53*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.5631570717145937},null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53]
[null,54,4.6031426571289193,4.4690705409018632,4.1637068436082387,3.9994459004783121,3.6701767042861317,3.5770738515776328,4.398496137176922,2.8614123843963806,4.705434088785017,null,null,null,54,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_54*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_54*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.5315163751457206},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_54*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_54*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.993537061672531},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_54*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_54*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.6031426571289193},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_54*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_54*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.6031426571289193},null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54]
[null,55,4.6431282425432441,4.5078914976148008,4.1917370557995275,4.0300377265580476,3.6995095492807946,3.6007353040666867,4.4362498738379754,2.8862682834688744,4.746308237314218,null,null,null,55,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_55*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_55*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.5707208134964006},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_55*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_55*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.0282272568672148},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_55*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_55*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.6431282425432441},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_55*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_55*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.6431282425432441},null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55]
[null,56,4.6831138279575697,4.5467124543277375,4.2197672679908163,4.0606295526377822,3.7288423942754574,3.6243967565557416,4.4739964049181919,2.9111241825413687,4.7871823858434199,null,null,null,56,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_56*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_56*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.6099227298937873},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_56*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_56*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.0629174520618996},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_56*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_56*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.6831138279575697},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_56*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_56*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.6831138279575697},null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56]
[null,57,4.7230994133718953,4.5855334110406751,4.247797480182105,4.0912213787175178,3.7581752392701206,3.6480582090447959,4.5117357449619018,2.9359800816138635,4.8280565343726218,null,null,null,57,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_57*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_57*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.6491221294283971},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_57*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_57*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.0976076472565843},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_57*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_57*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.7230994133718953},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_57*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_57*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.7230994133718953},null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57]
[null,58,4.76308499878622,4.6243543677536119,4.2758276923733947,4.1218132047972533,3.7875080842647839,3.6717196615338499,4.5494679084743135,2.9608359806863573,4.8689306829018228,null,null,null,58,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_58*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_58*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.6883190171770526},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_58*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_58*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.1322978424512682},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_58*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_58*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.76308499878622},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_58*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_58*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.76308499878622},null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58]
[null,59,4.8030705842005466,4.6631753244665495,4.3038579045646834,4.1524050308769889,3.8168409292594476,3.6953811140229047,4.5871929099216562,2.9856918797588525,4.9098048314310256,null,null,null,59,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_59*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_59*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.7275133982029347},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_59*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_59*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.1669880376459538},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_59*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_59*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.8030705842005466},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_59*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_59*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.8030705842005466},null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59]
[null,60,4.8430561696148713,4.7019962811794871,4.3318881167559722,4.1829968569567244,3.8461737742541109,3.7190425665119591,4.6249107637313003,3.0105477788313464,4.9506789799602267,null,null,null,60,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_60*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_10_60*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.7667052775556211},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_60*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_10_60*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.2016782328406377},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_60*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_10_60*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.8430561696148713},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_10_60*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_10_60*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.8430561696148713},null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60]
[]
[]
[]
[]
[]
["Busstørrelse","Hastighed (km/t)","Euro 6","EEV","Euro 5","Euro 4","Euro 3","Euro 2","Biodiesel","Ethanol","Gas",null,null,"Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol"]
["12 meter",10,2.4145968044826391,2.3442687422161543,2.4881277316560548,2.2529561203198263,2.020414898756397,2.1532437796832244,2.3179657093325736,1.5009652566318554,2.4682541821483621,null,null,"12 meter",10,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_10*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_10*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.3807759211801161},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_10*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_10*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.0948257627348648},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_10*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_10*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.4145968044826391},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_10*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_10*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.4145968044826391},"12 meter",10,null,null,null,null,"12 meter",10,null,null,null,null,"12 meter",10,null,null,null,null,"12 meter",10,null,null,null,null,"12 meter",10,null,null,null,null,"12 meter",10,null,null,null,null,"12 meter",10,null,null,null,null,"12 meter",10,null,null,null,null,"12 meter",10,null,null,null,null,"12 meter",10,null,null,null,null,"12 meter",10,null,null,null,null,"12 meter",10,null,null,null,null,"12 meter",10,null,null,null,null,"12 meter",10,null,null,null,null,"12 meter",10,null,null,null,null,"12 meter",10,null,null,null,null,"12 meter",10,null,null,null,null,"12 meter",10,null,null,null,null,"12 meter",10,null,null,null,null,"12 meter",10,null,null,null,null,"12 meter",10,null,null,null,null,"12 meter",10,null,null,null,null,"12 meter",10,null,null,null,null,"12 meter",10]
[null,{"$f":"B62+1","v":11},2.448547803523454,2.377230877207237,2.5119276509859674,2.2789310572159049,2.0453208587907192,2.1733342683539836,2.3503036361498748,1.5220699271481088,2.5029596432071339,null,null,null,11,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_11*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_11*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.4141623449427012},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_11*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_11*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.1242805467920833},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_11*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_11*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.448547803523454},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_11*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_11*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.448547803523454},null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11]
[null,{"$f":"B63+1","v":12},2.4824988025642689,2.4101930121983193,2.5357275703158804,2.304905994111984,2.0702268188250419,2.1934247570247427,2.3826348668168351,1.5431745976643623,2.5376651042659053,null,null,null,12,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_12*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_12*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.4475464250526673},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_12*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_12*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.1537353308493019},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_12*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_12*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.4824988025642689},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_12*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_12*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.4824988025642689},null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12]
[null,13,2.5164498016050834,2.4431551471894015,2.5595274896457934,2.3308809310080627,2.0951327788593646,2.2135152456955014,2.4149594152618494,1.5642792681806155,2.5723705653246762,null,null,null,13,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_13*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_13*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.4809281663849516},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_13*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_13*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.1831901149065196},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_13*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_13*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.5164498016050834},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_13*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_13*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.5164498016050834},null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13]
[null,14,2.5504008006458982,2.4761172821804838,2.5833274089757063,2.3568558679041414,2.1200387388936868,2.2336057343662605,2.4472772953747097,1.5853839386968691,2.607076026383448,null,null,null,14,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_14*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_14*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.5143075738009824},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_14*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_14*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.2126448989637382},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_14*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_14*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.5504008006458982},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_14*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_14*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.5504008006458982},null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14]
[null,15,2.5843517996867136,2.5090794171715665,2.6071273283056189,2.3828308048002205,2.1449446989280094,2.2536962230370197,2.4795885210067392,1.6064886092131228,2.6417814874422199,null,null,null,15,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_15*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_15*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.5476846521487224},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_15*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_15*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.2420996830209567},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_15*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_15*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.5843517996867136},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_15*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_15*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.5843517996867136},null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15]
[null,16,2.618302798727528,2.5420415521626487,2.6309272476355319,2.4088057416962991,2.1698506589623321,2.2737867117077784,2.5118931059709251,1.627593279729376,2.6764869485009908,null,null,null,16,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_16*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_16*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.581059406262717},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_16*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_16*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.2715544670781749},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_16*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_16*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.618302798727528},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_16*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_16*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.618302798727528},null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16]
[null,17,2.6522537977683429,2.575003687153731,2.6547271669654449,2.4347806785923778,2.1947566189966543,2.2938772003785375,2.5441910640420513,1.6486979502456294,2.7111924095597626,null,null,null,17,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_17*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_17*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.6144318409641407},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_17*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_17*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.301009251135393},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_17*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_17*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.6522537977683429},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_17*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_17*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.6522537977683429},null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17]
[null,18,2.6862047968091578,2.6079658221448132,2.6785270862953574,2.4607556154884564,2.219662579030977,2.3139676890492966,2.5764824089568314,1.6698026207618828,2.745897870618534,null,null,null,18,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_18*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_18*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.6478019610608436},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_18*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_18*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.3304640351926116},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_18*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_18*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.6862047968091578},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_18*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_18*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.6862047968091578},null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18]
[null,19,2.7201557958499722,2.6409279571358999,2.7023270056252704,2.4867305523845356,2.2445685390652996,2.3340581777200553,2.6087671544140383,1.690907291278136,2.7806033316773049,null,null,null,19,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_19*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_19*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.6811697713473954},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_19*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_19*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.3599188192498297},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_19*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_19*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.7201557958499722},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_19*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_19*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.7201557958499722},null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19]
[null,20,2.7541067948907876,2.6738900921269781,2.7261269249551834,2.5127054892806142,2.2694744990996218,2.3541486663908144,2.6410453140746375,1.7120119617943899,2.8153087927360771,null,null,null,20,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_20*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_20*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.7145352766051349},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_20*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_20*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.3893736033070487},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_20*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_20*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.7541067948907876},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_20*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_20*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.7541067948907876},null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20]
[null,21,2.788057793931602,2.7068522271180604,2.7499268442850964,2.5386804261766933,2.2943804591339445,2.3742391550615736,2.6733169015619134,1.7331166323106431,2.8500142537948481,null,null,null,21,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_21*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_21*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.7478984816022112},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_21*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_21*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.4188283873642664},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_21*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_21*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.788057793931602},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_21*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_21*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.788057793931602},null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21]
[null,22,2.8220087929724169,2.7398143621091426,2.7737267636150089,2.564655363072772,2.3192864191682672,2.3943296437323327,2.7055819304616033,1.7542213028268965,2.8847197148536194,null,null,null,22,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_22*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_22*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.7812593910936321},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_22*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_22*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.448283171421485},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_22*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_22*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.8220087929724169},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_22*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_22*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.8220087929724169},null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22]
[null,23,2.8559597920132322,2.7727764971002253,2.7975266829449219,2.5906302999688506,2.3441923792025898,2.4144201324030914,2.7378404143220267,1.7753259733431503,2.9194251759123917,null,null,null,23,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_23*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_23*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.8146180098213103},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_23*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_23*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.4777379554787036},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_23*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_23*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.8559597920132322},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_23*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_23*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.8559597920132322},null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23]
[null,24,2.8899107910540462,2.8057386320913071,2.8213266022748344,2.6166052368649293,2.369098339236912,2.4345106210738505,2.7700923666542092,1.7964306438594031,2.9541306369711622,null,null,null,24,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_24*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_24*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.8479743425141031},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_24*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_24*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.5071927395359213},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_24*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_24*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.8899107910540462},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_24*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_24*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.8899107910540462},null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24]
[null,25,2.9238617900948616,2.8387007670823898,2.8451265216047474,2.642580173761008,2.3940042992712347,2.4546011097446097,2.8023378009320163,1.817535314375657,2.988836098029934,null,null,null,25,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_25*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_25*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.8813283938878658},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_25*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_25*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.5366475235931398},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_25*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_25*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.9238617900948616},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_25*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_25*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.9238617900948616},null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25]
[null,26,2.957812789135676,2.8716629020734721,2.8689264409346604,2.6685551106570871,2.4189102593055569,2.4746915984153688,2.8345767305922775,1.8386399848919102,3.0235415590887054,null,null,null,26,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_26*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_26*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.9146801686454866},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_26*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_26*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.566102307650358},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_26*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_26*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.957812789135676},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_26*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_26*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.957812789135676},null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26]
[null,27,2.9917637881764909,2.9046250370645543,2.8927263602645734,2.6945300475531657,2.4438162193398796,2.4947820870861275,2.8668091690349158,1.8597446554081636,3.0582470201474767,null,null,null,27,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_27*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_27*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.9480296714769398},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_27*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_27*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.5955570917075761},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_27*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_27*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.9917637881764909},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_27*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_27*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.9917637881764909},null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27]
[null,28,3.0257147872173062,2.937587172055637,2.916526279594486,2.7205049844492448,2.4687221793742022,2.5148725757568866,2.8990351296230714,1.8808493259244172,3.0929524812062485,null,null,null,28,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_28*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_28*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.9813769070593237},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_28*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_28*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.6250118757647951},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_28*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_28*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.0257147872173062},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_28*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_28*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.0257147872173062},null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28]
[null,29,3.0596657862581207,2.9705493070467193,2.9403261989243989,2.7464799213453235,2.4936281394085249,2.5349630644276457,2.9312546256832315,1.9019539964406704,3.1276579422650199,null,null,null,29,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_29*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_29*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.0147218800569098},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_29*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_29*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.6544666598220132},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_29*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_29*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.0596657862581207},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_29*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_29*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.0596657862581207},null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29]
[null,30,3.0936167852989356,3.0035114420378015,2.9641261182543115,2.7724548582414021,2.5185340994428471,2.5550535530984044,2.9634676705053526,1.9230586669569241,3.1623634033237913,null,null,null,30,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_30*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_30*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.0480645951211818},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_30*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_30*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.6839214438792318},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_30*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_30*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.0936167852989356},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_30*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_30*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.0936167852989356},null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30]
[null,31,3.1275677843397509,3.0364735770288842,2.9879260375842245,2.7984297951374808,2.5434400594771698,2.5751440417691636,2.9956742773429892,1.9441633374731777,3.1970688643825631,null,null,null,31,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_31*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_31*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.0814050568908842},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_31*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_31*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.7133762279364504},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_31*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_31*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1275677843397509},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_31*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_31*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1275677843397509},null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31]
[null,32,3.1615187833805649,3.069435712019966,3.0117259569141375,2.8244047320335599,2.568346019511492,2.5952345304399227,3.0278744594134124,1.9652680079894307,3.231774325441334,null,null,null,32,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_32*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_32*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.1147432699920614},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_32*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_32*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.7428310119936681},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_32*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_32*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1615187833805649},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_32*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_32*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1615187833805649},null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32]
[null,33,3.1954697824213802,3.1023978470110487,3.0355258762440505,2.8503796689296386,2.5932519795458147,2.6153250191106814,3.0600682298977415,1.9863726785056843,3.2664797865001058,null,null,null,33,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_33*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_33*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.1480792390381067},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_33*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_33*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.7722857960508867},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_33*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_33*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1954697824213802},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_33*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_33*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1954697824213802},null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33]
[null,34,3.2294207814621947,3.135359982002131,3.0593257955739634,2.8763546058257172,2.6181579395801373,2.6354155077814405,3.0922556019410612,2.0074773490219378,3.3011852475588768,null,null,null,34,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_34*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_34*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.1814129686297981},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_34*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_34*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.8017405801081048},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_34*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_34*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.2294207814621947},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_34*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_34*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.2294207814621947},null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34]
[null,35,3.2633717805030096,3.1683221169932132,3.083125714903876,2.9023295427217963,2.64306389961446,2.6555059964521996,3.1244365886525487,2.0285820195381912,3.3358907086176486,null,null,null,35,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_35*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_35*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.2147444633553484},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_35*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_35*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.8311953641653234},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_35*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_35*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.2633717805030096},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_35*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_35*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.2633717805030096},null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35]
[null,36,3.2973227795438249,3.2012842519842959,3.106925634233789,2.928304479617875,2.6679698596487822,2.6755964851229583,3.1566112031055948,2.0496866900544446,3.3705961696764204,null,null,null,36,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_36*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_36*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.2480737277904446},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_36*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_36*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.8606501482225419},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_36*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_36*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.2973227795438249},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_36*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_36*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.2973227795438249},null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36]
[null,37,3.3312737785846389,3.2342463869753777,3.1307255535637015,2.9542794165139536,2.6928758196831049,2.6956869737937175,3.1887794583379239,2.0707913605706976,3.4053016307351909,null,null,null,37,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_37*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_37*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.2814007664982885},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_37*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_37*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.8901049322797592},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_37*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_37*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.3312737785846389},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_37*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_37*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.3312737785846389},null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37]
[null,38,3.3652247776254542,3.2672085219664604,3.1545254728936145,2.9802543534100323,2.7177817797174271,2.7157774624644766,3.22094136735172,2.0918960310869514,3.4400070917939631,null,null,null,38,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_38*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_38*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.314725584029647},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_38*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_38*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.9195597163369782},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_38*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_38*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.3652247776254542},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_38*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_38*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.3652247776254542},null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38]
[null,39,3.3991757766662687,3.3001706569575426,3.1783253922235275,3.0062292903061114,2.7426877397517497,2.7358679511352357,3.2530969431137433,2.1130007016032049,3.4747125528527341,null,null,null,39,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_39*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_39*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.3480481849228849},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_39*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_39*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.9490145003941963},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_39*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_39*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.3991757766662687},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_39*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_39*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.3991757766662687},null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39]
[null,40,3.4331267757070836,3.3331327919486249,3.2021253115534405,3.0322042272021901,2.7675936997860724,2.7559584398059949,3.2852461985554533,2.1341053721194583,3.5094180139115054,null,null,null,40,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_40*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_40*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.3813685737040133},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_40*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_40*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.9784692844514149},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_40*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_40*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.4331267757070836},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_40*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_40*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.4331267757070836},null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40]
[null,41,3.4670777747478989,3.3660949269397076,3.225925230883353,3.0581791640982692,2.7924996598203951,2.7760489284767536,3.3173891465731296,2.1552100426357117,3.5441234749702777,null,null,null,41,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_41*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_41*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.4146867548867297},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_41*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_41*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.0079240685086335},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_41*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_41*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.4670777747478989},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_41*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_41*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.4670777747478989},null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41]
[null,42,3.5010287737887134,3.3990570619307898,3.249725150213266,3.0841541009943478,2.8174056198547173,2.7961394171475127,3.3495258000279873,2.1763147131519651,3.5788289360290486,null,null,null,42,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_42*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_42*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.4480027329724594},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_42*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_42*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.0373788525658512},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_42*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_42*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.5010287737887134},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_42*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_42*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.5010287737887134},null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42]
[null,43,3.5349797728295282,3.4320191969218721,3.2735250695431786,3.1101290378904265,2.8423115798890399,2.8162299058182718,3.3816561717463012,2.1974193836682185,3.61353439708782,null,null,null,43,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_43*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_43*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.4813165124503991},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_43*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_43*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.0668336366230697},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_43*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_43*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.5349797728295282},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_43*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_43*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.5349797728295282},null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43]
[null,44,3.5689307718703436,3.4649813319129548,3.2973249888730916,3.1361039747865052,2.8672175399233621,2.8363203944890305,3.4137802745195218,2.2185240541844724,3.6482398581465922,null,null,null,44,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_44*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_44*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.5146280977975559},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_44*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_44*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.0962884206802883},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_44*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_44*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.5689307718703436},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_44*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_44*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.5689307718703436},null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44]
[null,45,3.6028817709111576,3.4979434669040366,3.3211249082030045,3.1620789116825838,2.8921234999576848,2.8564108831597896,3.445898121104392,2.2396287247007254,3.6829453192053627,null,null,null,45,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_45*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_45*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.5479374934787895},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_45*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_45*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.1257432047375064},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_45*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_45*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.6028817709111576},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_45*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_45*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.6028817709111576},null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45]
[null,46,3.6368327699519729,3.5309056018951193,3.3449248275329175,3.1880538485786629,2.9170294599920075,2.8765013718305488,3.4780097242230674,2.2607333952169788,3.717650780264135,null,null,null,46,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_46*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_46*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.5812447039468558},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_46*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_46*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.155197988794725},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_46*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_46*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.6368327699519729},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_46*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_46*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.6368327699519729},null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46]
[null,47,3.6707837689927874,3.5638677368862015,3.3687247468628305,3.214028785474742,2.9419354200263301,2.8965918605013075,3.5101150965632337,2.2818380657332322,3.7523562413229059,null,null,null,47,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_47*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_47*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.6145497336424435},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_47*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_47*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.1846527728519431},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_47*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_47*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.6707837689927874},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_47*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_47*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.6707837689927874},null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47]
[null,48,3.7047347680336022,3.5968298718772838,3.3925246661927431,3.2400037223708207,2.9668413800606523,2.9166823491720666,3.5422142507782199,2.3029427362494856,3.7870617023816773,null,null,null,48,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_48*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_48*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.6478525869942184},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_48*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_48*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.2141075569091613},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_48*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_48*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.7047347680336022},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_48*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_48*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.7047347680336022},null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48]
[null,49,3.7386857670744176,3.6297920068683664,3.4163245855226556,3.2659786592668993,2.991747340094975,2.9367728378428257,3.5743071994871185,2.3240474067657395,3.8217671634404495,null,null,null,49,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_49*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_49*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.6811532684188624},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_49*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_49*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.2435623409663803},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_49*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_49*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.7386857670744176},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_49*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_49*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.7386857670744176},null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49]
[null,50,3.7726367661152316,3.6627541418594483,3.4401245048525686,3.291953596162978,3.0166533001292972,2.9568633265135844,3.6063939552748976,2.345152077281992,3.85647262449922,null,null,null,50,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_50*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_50*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.7144517823211149},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_50*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_50*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.273017125023598},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_50*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_50*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.7726367661152316},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_50*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_50*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.7726367661152316},null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50]
[null,51,3.8065877651560469,3.6957162768505309,3.4639244241824816,3.3179285330590567,3.0415592601636199,2.976953815184344,3.6384745306925201,2.3662567477982459,3.8911780855579918,null,null,null,51,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_51*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_51*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.7477481330938125},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_51*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_51*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.3024719090808166},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_51*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_51*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.8065877651560469},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_51*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_51*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.8065877651560469},null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51]
[null,52,3.8405387641968618,3.7286784118416132,3.4877243435123946,3.3439034699551358,3.0664652201979425,2.9970443038551027,3.6705489382570544,2.3873614183144993,3.9258835466167636,null,null,null,52,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_52*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_52*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.7810423251179293},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_52*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_52*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.3319266931380351},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_52*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_52*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.8405387641968618},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_52*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_52*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.8405387641968618},null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52]
[null,53,3.8744897632376762,3.7616405468326954,3.5115242628423076,3.3698784068512144,3.0913711802322652,3.0171347925258614,3.7026171904517922,2.4084660888307527,3.9605890076755346,null,null,null,53,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_53*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_53*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.8143343627626169},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_53*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_53*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.3613814771952528},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_53*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_53*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.8744897632376762},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_53*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_53*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.8744897632376762},null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53]
[null,54,3.9084407622784916,3.7946026818237781,3.5353241821722201,3.3958533437472935,3.1162771402665879,3.0372252811966209,3.7346792997263605,2.4295707593470066,3.9952944687343064,null,null,null,54,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_54*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_54*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.8476242503852456},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_54*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_54*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.3908362612524723},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_54*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_54*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.9084407622784916},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_54*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_54*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.9084407622784916},null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54]
[null,55,3.942391761319306,3.8275648168148604,3.5591241015021331,3.4218282806433722,3.1411831003009101,3.0573157698673796,3.7667352784968346,2.4506754298632596,4.0299999297930773,null,null,null,55,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_55*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_55*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.8809119923314412},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_55*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_55*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.42029104530969},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_55*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_55*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.942391761319306},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_55*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_55*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.942391761319306},null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55]
[null,56,3.9763427603601209,3.8605269518059426,3.5829240208320456,3.4478032175394508,3.1660890603352323,3.0774062585381388,3.7987851391458523,2.471780100379513,4.0647053908518487,null,null,null,56,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_56*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_56*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.9141975929351265},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_56*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_56*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.4497458293669081},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_56*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_56*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.9763427603601209},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_56*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_56*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.9763427603601209},null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56]
[null,57,4.0102937594009358,3.8934890867970253,3.6067239401619586,3.4737781544355295,3.190995020369555,3.0974967472088979,3.8308288940227269,2.4928847708957664,4.0994108519106209,null,null,null,57,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_57*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_57*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.9474810565185625},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_57*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_57*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.4792006134241262},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_57*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_57*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.0102937594009358},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_57*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_57*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.0102937594009358},null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57]
[null,58,4.0442447584417502,3.9264512217881071,3.6305238594918716,3.4997530913316082,3.2159009804038776,3.1175872358796566,3.8628665554435546,2.5139894414120199,4.1341163129693914,null,null,null,58,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_58*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_58*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.9807623873923816},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_58*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_58*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.5086553974813444},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_58*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_58*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.0442447584417502},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_58*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_58*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.0442447584417502},null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58]
[null,59,4.0781957574825656,3.9594133567791898,3.6543237788217846,3.5257280282276873,3.2408069404382003,3.1376777245504157,3.8948981356913359,2.5350941119282733,4.1688217740281637,null,null,null,59,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_59*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_59*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.0140415898556352},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_59*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_59*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.5381101815385634},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_59*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_59*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.0781957574825656},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_59*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_59*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.0781957574825656},null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59]
[null,60,4.11214675652338,3.9923754917702721,3.6781236981516972,3.5517029651237664,3.2657129004725229,3.1577682132211748,3.9269236470160753,2.5561987824445267,4.203527235086935,null,null,null,60,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_60*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_12_60*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.0473186681958238},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_60*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_12_60*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.5675649655957815},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_60*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_12_60*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.11214675652338},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_12_60*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_12_60*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.11214675652338},null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60]
[]
[]
[]
[]
["Busstørrelse","Hastighed (km/t)","Euro 6","EEV","Euro 5","Euro 4","Euro 3","Euro 2","Biodiesel","Ethanol","Gas",null,null,"Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol"]
["13,7 meter",10,1.9925252830590736,1.9344905660767704,2.0532030041625764,1.8591393904879205,1.6672463744537787,1.7768567669945967,1.9127853033412396,1.2385965297726069,2.0368033511088282,null,null,"13,7 meter",10,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_10*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_10*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.9646162901578319},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_10*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_10*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.7286502194088103},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_10*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_10*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.9925252830590736},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_10*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_10*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.9925252830590736},"13,7 meter",10,null,null,null,null,"13,7 meter",10,null,null,null,null,"13,7 meter",10,null,null,null,null,"13,7 meter",10,null,null,null,null,"13,7 meter",10,null,null,null,null,"13,7 meter",10,null,null,null,null,"13,7 meter",10,null,null,null,null,"13,7 meter",10,null,null,null,null,"13,7 meter",10,null,null,null,null,"13,7 meter",10,null,null,null,null,"13,7 meter",10,null,null,null,null,"13,7 meter",10,null,null,null,null,"13,7 meter",10,null,null,null,null,"13,7 meter",10,null,null,null,null,"13,7 meter",10,null,null,null,null,"13,7 meter",10,null,null,null,null,"13,7 meter",10,null,null,null,null,"13,7 meter",10,null,null,null,null,"13,7 meter",10,null,null,null,null,"13,7 meter",10,null,null,null,null,"13,7 meter",10,null,null,null,null,"13,7 meter",10,null,null,null,null,"13,7 meter",10,null,null,null,null,"13,7 meter",10]
[null,{"$f":"B118+1","v":11},2.0205416474675539,1.9616909198714119,2.0728426975936203,1.8805739084145645,1.6877987726741013,1.7934354382457072,1.9394705605508766,1.2560121038826193,2.0654422975745264,null,null,null,11,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_11*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_11*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.9921667670467169},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_11*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_11*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.7529563072128269},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_11*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_11*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.0205416474675539},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_11*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_11*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.0205416474675539},null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11]
[null,{"$f":"B119+1","v":12},2.0485580118760347,1.9888912736660529,2.0924823910246642,1.9020084263412091,1.7083511708944243,1.8100141094968176,1.9661502920972522,1.2734276779926319,2.094081244040225,null,null,null,12,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_12*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_12*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.0197153099534608},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_12*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_12*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.7772623950168436},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_12*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_12*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.0485580118760347},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_12*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_12*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.0485580118760347},null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12]
[null,13,2.0765743762845146,2.0160916274606939,2.1121220844557085,1.9234429442678531,1.7289035691147501,1.8265927807479276,1.992824509474078,1.2908432521026438,2.1227201905059228,null,null,null,13,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_13*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_13*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.0472619229008617},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_13*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_13*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.8015684828208598},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_13*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_13*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.0765743762845146},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_13*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_13*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.0765743762845146},null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13]
[null,14,2.1045907406929949,2.0432919812553352,2.1317617778867528,1.9448774621944973,1.7494559673350703,1.8431714519990381,2.0194932241432104,1.3082588262126562,2.151359136971621,null,null,null,14,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_14*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_14*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.0748066099005702},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_14*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_14*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.8258745706248762},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_14*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_14*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.1045907406929949},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_14*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_14*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.1045907406929949},null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14]
[null,15,2.1326071051014757,2.0704923350499764,2.1514014713177967,1.9663119801211417,1.7700083655553933,1.8597501232501485,2.0461564475347611,1.3256744003226686,2.1799980834373196,null,null,null,15,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_15*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_15*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.1023493749531257},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_15*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_15*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.8501806584288931},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_15*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_15*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.1326071051014757},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_15*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_15*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.1326071051014757},null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15]
[null,16,2.160623469509956,2.0976926888446177,2.1710411647488406,1.9877464980477859,1.7905607637757164,1.8763287945012586,2.0728141910472071,1.343089974432681,2.2086370299030178,null,null,null,16,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_16*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_16*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.1298902220479938},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_16*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_16*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.8744867462329098},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_16*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_16*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.160623469509956},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_16*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_16*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.160623469509956},null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16]
[null,17,2.1886398339184363,2.1248930426392585,2.1906808581798849,2.0091810159744301,1.811113161996039,1.892907465752369,2.0994664660475006,1.3605055485426933,2.2372759763687156,null,null,null,17,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_17*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_17*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.1574291551636087},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_17*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_17*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.8987928340369262},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_17*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_17*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.1886398339184363},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_17*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_17*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.1886398339184363},null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17]
[null,18,2.2166561983269166,2.1520933964338997,2.2103205516109288,2.0306155339010741,1.8316655602163621,1.9094861370034795,2.1261132838711769,1.3779211226527055,2.2659149228344138,null,null,null,18,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_18*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_18*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.1849661782674077},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_18*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_18*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.9230989218409429},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_18*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_18*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.2166561983269166},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_18*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_18*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.2166561983269166},null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18]
[null,19,2.2446725627353969,2.1792937502285445,2.2299602450419731,2.0520500518277185,1.8522179584366851,1.9260648082545895,2.1527546558224642,1.3953366967627179,2.294553869300112,null,null,null,19,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_19*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_19*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.2125012953158705},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_19*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_19*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.9474050096449593},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_19*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_19*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.2446725627353969},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_19*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_19*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.2446725627353969},null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19]
[null,20,2.2726889271438777,2.2064941040231822,2.249599938473017,2.0734845697543625,1.8727703566570078,1.9426434795056999,2.1793905931743907,1.4127522708727305,2.3231928157658106,null,null,null,20,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_20*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_20*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.2400345102545574},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_20*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_20*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.9717110974489762},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_20*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_20*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.2726889271438777},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_20*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_20*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.2726889271438777},null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20]
[null,21,2.3007052915523576,2.2336944578178231,2.2692396319040613,2.0949190876810073,1.8933227548773308,1.9592221507568104,2.2060211071688909,1.4301678449827424,2.3518317622315084,null,null,null,21,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_21*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_21*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.267565827018144},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_21*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_21*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.9960171852529922},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_21*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_21*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.3007052915523576},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_21*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_21*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.3007052915523576},null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21]
[null,22,2.3287216559608384,2.2608948116124643,2.2888793253351052,2.1163536056076513,1.9138751530976539,1.9758008220079208,2.2326462090169148,1.447583419092755,2.380470708697207,null,null,null,22,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_22*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_22*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.2950952495304651},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_22*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_22*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.0203232730570093},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_22*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_22*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.3287216559608384},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_22*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_22*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.3287216559608384},null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22]
[null,23,2.3567380203693191,2.2880951654071056,2.3085190187661495,2.1377881235342953,1.9344275513179769,1.9923794932590309,2.2592659098985362,1.4649989932027676,2.4091096551629052,null,null,null,23,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_23*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_23*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.3226227817045451},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_23*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_23*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.044629360861026},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_23*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_23*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.3567380203693191},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_23*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_23*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.3567380203693191},null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23]
[null,24,2.3847543847777986,2.3152955192017464,2.3281587121971934,2.1592226414609397,1.9549799495382996,2.0089581645101413,2.2858802209630533,1.4824145673127793,2.4377486016286025,null,null,null,24,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_24*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_24*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.3501484274426376},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_24*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_24*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.0689354486650418},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_24*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_24*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.3847543847777986},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_24*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_24*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.3847543847777986},null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24]
[null,25,2.4127707491862798,2.3424958729963881,2.3477984056282373,2.1806571593875836,1.9755323477586226,2.0255368357612515,2.3124891533290999,1.4998301414227921,2.4663875480943016,null,null,null,25,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_25*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_25*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.3776721906362668},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_25*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_25*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.0932415364690593},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_25*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_25*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.4127707491862798},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_25*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_25*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.4127707491862798},null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25]
[null,26,2.4407871135947596,2.3696962267910289,2.3674380990592816,2.2020916773142281,1.9960847459789455,2.0421155070123622,2.3390927180847472,1.5172457155328041,2.4950264945599994,null,null,null,26,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_26*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_26*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.4051940751662553},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_26*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_26*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.1175476242730751},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_26*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_26*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.4407871135947596},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_26*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_26*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.4407871135947596},null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26]
[null,27,2.46880347800324,2.3968965805856701,2.3870777924903259,2.223526195240872,2.0166371441992683,2.058694178263472,2.3656909262876122,1.5346612896428165,2.5236654410256976,null,null,null,27,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_27*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_27*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.4327140849027704},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_27*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_27*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.1418537120770917},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_27*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_27*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.46880347800324},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_27*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_27*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.46880347800324},null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27]
[null,28,2.4968198424117207,2.4240969343803114,2.4067174859213698,2.2449607131675164,2.0371895424195916,2.0752728495145827,2.3922837889649582,1.5520768637528288,2.5523043874913962,null,null,null,28,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_28*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_28*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.4602322237053538},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_28*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_28*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.1661597998811084},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_28*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_28*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.4968198424117207},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_28*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_28*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.4968198424117207},null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28]
[null,29,2.524836206820201,2.4512972881749526,2.4263571793524137,2.2663952310941609,2.0577419406399144,2.0918515207656929,2.4188713171138025,1.5694924378628412,2.5809433339570944,null,null,null,29,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_29*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_29*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.4877484954229616},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_29*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_29*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.1904658876851251},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_29*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_29*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.524836206820201},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_29*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_29*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.524836206820201},null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29]
[null,30,2.5528525712286814,2.4784976419695934,2.4459968727834576,2.2878297490208048,2.0782943388602373,2.1084301920168032,2.4454535217010167,1.5869080119728536,2.6095822804227922,null,null,null,30,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_30*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_30*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.5152629038939986},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_30*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_30*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.2147719754891417},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_30*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_30*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.5528525712286814},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_30*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_30*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.5528525712286814},null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30]
[null,31,2.5808689356371621,2.5056979957642351,2.4656365662145019,2.3092642669474488,2.0988467370805601,2.1250088632679134,2.4720304136634343,1.604323586082866,2.6382212268884908,null,null,null,31,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_31*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_31*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.5427754529463575},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_31*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_31*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.2390780632931584},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_31*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_31*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.5808689356371621},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_31*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_31*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.5808689356371621},null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31]
[null,32,2.608885300045642,2.5328983495588759,2.4852762596455462,2.3306987848740937,2.119399135300883,2.1415875345190241,2.4986020039079477,1.6217391601928781,2.6668601733541886,null,null,null,32,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_32*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_32*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.5702861463974491},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_32*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_32*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.2633841510971746},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_32*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_32*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.608885300045642},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_32*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_32*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.608885300045642},null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32]
[null,33,2.6369016644541228,2.5600987033535172,2.5049159530765901,2.3521333028007376,2.1399515335212063,2.1581662057701343,2.5251683033116161,1.6391547343028907,2.6954991198198872,null,null,null,33,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_33*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_33*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.5977949880542455},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_33*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_33*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.2876902389011917},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_33*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_33*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.6369016644541228},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_33*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_33*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.6369016644541228},null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33]
[null,34,2.6649180288626027,2.5872990571481584,2.5245556465076344,2.3735678207273816,2.1605039317415291,2.1747448770212445,2.5517293227217634,1.6565703084129026,2.724138066285585,null,null,null,34,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_34*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_34*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.6253019817133088},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_34*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_34*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.3119963267052075},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_34*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_34*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.6649180288626027},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_34*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_34*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.6649180288626027},null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34]
[null,35,2.6929343932710834,2.6144994109427993,2.5441953399386783,2.395002338654026,2.1810563299618524,2.1913235482723548,2.5782850729560831,1.6739858825229152,2.7527770127512836,null,null,null,35,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_35*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_35*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.6528071311608334},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_35*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_35*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.3363024145092246},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_35*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_35*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.6929343932710834},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_35*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_35*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.6929343932710834},null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35]
[null,36,2.7209507576795642,2.6416997647374409,2.5638350333697226,2.4164368565806704,2.2016087281821748,2.207902219523465,2.6048355648027366,1.6914014566329278,2.7814159592169818,null,null,null,36,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_36*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_36*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.6803104401726743},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_36*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_36*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.3606085023132413},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_36*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_36*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.7209507576795642},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_36*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_36*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.7209507576795642},null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36]
[null,37,2.7489671220880436,2.6689001185320813,2.5834747268007665,2.4378713745073144,2.2221611264024981,2.2244808907745757,2.6313808090204547,1.7088170307429396,2.8100549056826791,null,null,null,37,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_37*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_37*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.7078119125143876},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_37*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_37*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.3849145901172575},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_37*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_37*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.7489671220880436},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_37*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_37*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.7489671220880436},null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37]
[null,38,2.7769834864965248,2.696100472326723,2.6031144202318104,2.4593058924339584,2.2427135246228205,2.2410595620256859,2.6579208163386392,1.7262326048529524,2.8386938521483782,null,null,null,38,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_38*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_38*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.735311551941265},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_38*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_38*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.4092206779212746},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_38*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_38*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.7769834864965248},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_38*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_38*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.7769834864965248},null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38]
[null,39,2.8049998509050047,2.7233008261213638,2.6227541136628547,2.4807404103606028,2.2632659228431438,2.2576382332767961,2.6844555974574607,1.7436481789629643,2.867332798614076,null,null,null,39,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_39*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_39*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.7628093621983645},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_39*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_39*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.4335267657252908},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_39*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_39*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.8049998509050047},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_39*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_39*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.8049998509050047},null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39]
[null,40,2.833016215313485,2.7505011799160051,2.642393807093899,2.5021749282872472,2.2838183210634666,2.2742169045279068,2.71098516304796,1.7610637530729767,2.8959717450797742,null,null,null,40,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_40*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_40*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.7903053470205514},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_40*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_40*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.457832853529307},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_40*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_40*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.833016215313485},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_40*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_40*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.833016215313485},null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40]
[null,41,2.8610325797219658,2.7777015337106463,2.6620335005249429,2.5236094462138916,2.3043707192837899,2.290795575779017,2.7375095237521463,1.7784793271829891,2.9246106915454728,null,null,null,41,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_41*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_41*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.8177995101325291},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_41*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_41*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.4821389413333241},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_41*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_41*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.8610325797219658},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_41*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_41*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.8610325797219658},null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41]
[null,42,2.8890489441304461,2.8049018875052876,2.6816731939559868,2.5450439641405356,2.3249231175041123,2.3073742470301273,2.7640286901830948,1.7958949012930014,2.953249638011171,null,null,null,42,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_42*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_42*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.8452918552488731},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_42*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_42*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.5064450291373408},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_42*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_42*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.8890489441304461},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_42*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_42*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.8890489441304461},null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42]
[null,43,2.9170653085389264,2.8321022412999288,2.7013128873870307,2.5664784820671795,2.3454755157244356,2.3239529182812375,2.7905426729250475,1.8133104754030138,2.9818885844768688,null,null,null,43,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_43*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_43*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.8727823860740687},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_43*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_43*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.530751116941357},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_43*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_43*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.9170653085389264},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_43*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_43*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.9170653085389264},null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43]
[null,44,2.9450816729474072,2.8593025950945701,2.720952580818075,2.587912999993824,2.3660279139447584,2.3405315895323477,2.8170514825335093,1.8307260495130262,3.0105275309425674,null,null,null,44,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_44*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_44*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.9002711063025428},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_44*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_44*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.5550572047453737},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_44*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_44*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.9450816729474072},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_44*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_44*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.9450816729474072},null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44]
[null,45,2.9730980373558871,2.8865029488892109,2.7405922742491193,2.6093475179204679,2.3865803121650813,2.3571102607834584,2.8435551295353441,1.8481416236230384,3.0391664774082652,null,null,null,45,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_45*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_45*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.9277580196186967},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_45*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_45*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.5793632925493899},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_45*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_45*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.9730980373558871},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_45*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_45*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.9730980373558871},null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45]
[null,46,3.0011144017643678,2.9137033026838521,2.7602319676801632,2.6307820358471123,2.4071327103854046,2.3736889320345687,2.8700536244288748,1.865557197733051,3.0678054238739638,null,null,null,46,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_46*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_46*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.955243129696945},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_46*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_46*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.603669380353407},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_46*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_46*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.0011144017643678},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_46*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_46*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.0011144017643678},null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46]
[null,47,3.0291307661728477,2.9409036564784934,2.7798716611112075,2.6522165537737568,2.4276851086057274,2.3902676032856789,2.8965469776839803,1.8829727718430629,3.0964443703396616,null,null,null,47,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_47*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_47*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.9827264402017439},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_47*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_47*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.6279754681574232},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_47*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_47*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.0291307661728477},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_47*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_47*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.0291307661728477},null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47]
[null,48,3.0571471305813285,2.9681040102731342,2.7995113545422514,2.6736510717004012,2.4482375068260502,2.4068462745367891,2.9230351997421868,1.9003883459530755,3.1250833168053602,null,null,null,48,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_48*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_48*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.0102079547876288},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_48*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_48*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.6522815559614399},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_48*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_48*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.0571471305813285},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_48*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_48*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.0571471305813285},null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48]
[null,49,3.0851634949898092,2.9953043640677759,2.8191510479732953,2.6950855896270451,2.4687899050463731,2.4234249457878998,2.94951830101677,1.9178039200630881,3.1537222632710584,null,null,null,49,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_49*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_49*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.0376876770992456},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_49*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_49*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.676587643765457},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_49*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_49*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.0851634949898092},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_49*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_49*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.0851634949898092},null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49]
[null,50,3.1131798593982887,3.0225047178624163,2.8387907414043392,2.7165201075536891,2.4893423032666959,2.4400036170390096,2.9759962918928453,1.9352194941730998,3.1823612097367557,null,null,null,50,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_50*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_50*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.0651656107713836},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_50*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_50*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.7008937315694728},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_50*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_50*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1131798593982887},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_50*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_50*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1131798593982887},null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50]
[null,51,3.1411962238067694,3.049705071657058,2.8584304348353835,2.7379546254803335,2.5098947014870188,2.4565822882901203,3.0024691827274674,1.9526350682831124,3.2110001562024544,null,null,null,51,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_51*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_51*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.0926417594290134},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_51*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_51*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.7251998193734894},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_51*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_51*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1411962238067694},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_51*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_51*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1411962238067694},null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51]
[null,52,3.1692125882152502,3.0769054254516988,2.8780701282664278,2.7593891434069779,2.5304470997073421,2.4731609595412305,3.0289369838497211,1.9700506423931248,3.239639102668153,null,null,null,52,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_52*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_52*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.1201161266873152},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_52*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_52*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.7495059071775065},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_52*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_52*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1692125882152502},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_52*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_52*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1692125882152502},null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52]
[null,53,3.1972289526237301,3.10410577924634,2.8977098216974722,2.7808236613336219,2.5509994979276649,2.4897396307923407,3.0553997055608186,1.9874662165031369,3.2682780491338508,null,null,null,53,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_53*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_53*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.1475887161517111},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_53*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_53*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.7738119949815228},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_53*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_53*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1972289526237301},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_53*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_53*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1972289526237301},null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53]
[null,54,3.2252453170322108,3.1313061330409813,2.9173495151285156,2.8022581792602663,2.5715518961479882,2.5063183020434514,3.0818573581341924,2.0048817906131493,3.2969169955995494,null,null,null,54,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_54*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_54*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.1750595314179044},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_54*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_54*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.798118082785539},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_54*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_54*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.2252453170322108},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_54*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_54*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.2252453170322108},null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54]
[null,55,3.2532616814406912,3.1585064868356225,2.9369892085595599,2.8236926971869103,2.5921042943683106,2.5228969732945616,3.1083099518155879,2.0222973647231619,3.3255559420652476,null,null,null,55,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_55*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_55*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.2025285760719049},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_55*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_55*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.8224241705895556},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_55*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_55*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.2532616814406912},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_55*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_55*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.2532616814406912},null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55]
[null,56,3.2812780458491715,3.1857068406302638,2.9566289019906038,2.8451272151135547,2.6126566925886334,2.5394756445456719,3.1347574968231569,2.0397129388331741,3.3541948885309454,null,null,null,56,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_56*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_56*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.2299958536900668},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_56*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_56*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.8467302583935727},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_56*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_56*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.2812780458491715},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_56*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_56*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.2812780458491715},null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56]
[null,57,3.3092944102576518,3.212907194424905,2.9762685954216481,2.8665617330401987,2.6332090908089567,2.5560543157967826,3.1612000033475538,2.0571285129431862,3.3828338349966436,null,null,null,57,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_57*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_57*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.2574613678391175},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_57*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_57*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.871036346197589},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_57*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_57*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.3092944102576518},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_57*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_57*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.3092944102576518},null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57]
[null,58,3.3373107746661321,3.2401075482195458,2.995908288852692,2.8879962509668426,2.6537614890292796,2.5726329870478923,3.187637481552021,2.0745440870531984,3.4114727814623418,null,null,null,58,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_58*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_58*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.284925122076193},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_58*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_58*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.8953424340016056},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_58*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_58*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.3373107746661321},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_58*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_58*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.3373107746661321},null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58]
[null,59,3.3653271390746129,3.2673079020141871,3.0155479822837363,2.9094307688934875,2.6743138872496028,2.589211658299003,3.21406994157249,2.091959661163211,3.4401117279280404,null,null,null,59,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_59*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_59*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.3123871199488697},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_59*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_59*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.9196485218056223},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_59*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_59*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.3653271390746129},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_59*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_59*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.3653271390746129},null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59]
[null,60,3.3933435034830928,3.2945082558088283,3.0351876757147802,2.9308652868201319,2.6948662854699257,2.6057903295501132,3.2404973935176651,2.1093752352732231,3.4687506743937382,null,null,null,60,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_60*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_13.7_60*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.339847364995193},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_60*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_13.7_60*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.9439546096096385},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_60*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_13.7_60*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.3933435034830928},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_13.7_60*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_13.7_60*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.3933435034830928},null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60]
[]
[]
[]
[]
[]
["Busstørrelse","Hastighed (km/t)","Euro 6","EEV","Euro 5","Euro 4","Euro 3","Euro 2","Biodiesel","Ethanol","Gas",null,null,"Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol"]
["14,6 meter",10,1.85764590556067,1.8035397141365763,1.9142161890722693,1.7332892616068551,1.5543859982092465,1.656576569461492,1.7833037388179223,1.1547526105371517,1.898926672494021,null,null,"14,6 meter",10,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_10*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_10*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.8316261472007085},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_10*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_10*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.6116332523024386},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_10*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_10*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.85764590556067},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_10*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_10*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.85764590556067},"14,6 meter",10,null,null,null,null,"14,6 meter",10,null,null,null,null,"14,6 meter",10,null,null,null,null,"14,6 meter",10,null,null,null,null,"14,6 meter",10,null,null,null,null,"14,6 meter",10,null,null,null,null,"14,6 meter",10,null,null,null,null,"14,6 meter",10,null,null,null,null,"14,6 meter",10,null,null,null,null,"14,6 meter",10,null,null,null,null,"14,6 meter",10,null,null,null,null,"14,6 meter",10,null,null,null,null,"14,6 meter",10,null,null,null,null,"14,6 meter",10,null,null,null,null,"14,6 meter",10,null,null,null,null,"14,6 meter",10,null,null,null,null,"14,6 meter",10,null,null,null,null,"14,6 meter",10,null,null,null,null,"14,6 meter",10,null,null,null,null,"14,6 meter",10,null,null,null,null,"14,6 meter",10,null,null,null,null,"14,6 meter",10,null,null,null,null,"14,6 meter",10,null,null,null,null,"14,6 meter",10]
[null,{"$f":"B175+1","v":11},1.8837657671627341,1.8288988030706157,1.9325264190095441,1.7532728195584844,1.5735471495020519,1.6720329860154537,1.8081825994355447,1.170989277752126,1.9256269719049763,null,null,null,11,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_11*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_11*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.8573116584582179},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_11*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_11*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.6342939958690212},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_11*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_11*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.8837657671627341},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_11*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_11*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.8837657671627341},null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11]
[null,{"$f":"B176+1","v":12},1.9098856287647947,1.8542578920046551,1.9508366489468194,1.7732563775101138,1.5927083007948577,1.6874894025694156,1.8330563084368641,1.1872259449671005,1.9523272713159316,null,null,null,12,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_12*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_12*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.882995366650019},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_12*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_12*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.6569547394356019},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_12*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_12*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.9098856287647947},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_12*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_12*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.9098856287647947},null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12]
[null,13,1.9360054903668549,1.8796169809386942,1.9691468788840947,1.793239935461743,1.6118694520876635,1.7029458191233771,1.8579248765375513,1.2034626121820748,1.9790275707268865,null,null,null,13,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_13*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_13*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.9086772755265984},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_13*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_13*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.6796154830021819},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_13*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_13*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.9360054903668549},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_13*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_13*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.9360054903668549},null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13]
[null,14,1.9621253519689155,1.9049760698727334,1.9874571088213699,1.8132234934133722,1.6310306033804691,1.718402235677339,1.8827883144235793,1.2196992793970494,2.005727870137842,null,null,null,14,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_14*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_14*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.9343573888280479},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_14*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_14*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.7022762265687623},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_14*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_14*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.9621253519689155},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_14*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_14*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.9621253519689155},null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14]
[null,15,1.9882452135709763,1.930335158806773,2.0057673387586448,1.8332070513650016,1.6501917546732747,1.7338586522313009,1.9076466327513248,1.2359359466120239,2.0324281695487976,null,null,null,15,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_15*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_15*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.9600357102840982},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_15*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_15*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.724936970135343},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_15*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_15*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.9882452135709763},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_15*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_15*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.9882452135709763},null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15]
[null,16,2.0143650751730364,1.9556942477408121,2.0240775686959203,1.8531906093166308,1.6693529059660805,1.7493150687852623,1.9324998421476716,1.2521726138269982,2.0591284689597522,null,null,null,16,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_16*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_16*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.9857122436141585},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_16*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_16*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.747597713701923},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_16*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_16*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.0143650751730364},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_16*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_16*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.0143650751730364},null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16]
[null,17,2.0404849367750968,1.9810533366748515,2.0423877986331953,1.87317416726826,1.6885140572588861,1.764771485339224,1.9573479532101119,1.2684092810419725,2.0858287683707073,null,null,null,17,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_17*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_17*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.0113869925273522},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_17*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_17*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.7702584572685034},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_17*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_17*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.0404849367750968},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_17*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_17*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.0404849367750968},null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17]
[null,18,2.0666047983771576,2.0064124256088904,2.0606980285704704,1.8931577252198892,1.707675208551692,1.7802279018931859,1.9821909765068488,1.284645948256947,2.1125290677816633,null,null,null,18,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_18*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_18*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.0370599607225497},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_18*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_18*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.7929192008350838},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_18*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_18*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.0666047983771576},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_18*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_18*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.0666047983771576},null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18]
[null,19,2.0927246599792175,2.0317715145429331,2.0790082585077454,1.9131412831715187,1.7268363598444976,1.7956843184471474,2.0070289225768962,1.3008826154719211,2.1392293671926179,null,null,null,19,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_19*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_19*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.0627311518884053},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_19*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_19*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.8155799444016638},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_19*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_19*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.0927246599792175},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_19*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_19*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.0927246599792175},null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19]
[null,20,2.1188445215812788,2.0571306034769696,2.0973184884450209,1.9331248411231479,1.7459975111373032,1.8111407350011093,2.0318618019301815,1.317119282686896,2.1659296666035739,null,null,null,20,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_20*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_20*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.0884005697033947},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_20*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_20*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.8382406879682449},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_20*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_20*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.1188445215812788},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_20*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_20*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.1188445215812788},null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20]
[null,21,2.1449643831833387,2.0824896924110088,2.1156287183822959,1.9531083990747773,1.765158662430109,1.826597151555071,2.0566896250476425,1.3333559499018701,2.1926299660145285,null,null,null,21,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_21*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_21*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.114068217835845},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_21*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_21*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.8609014315348249},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_21*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_21*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.1449643831833387},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_21*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_21*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.1449643831833387},null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21]
[null,22,2.1710842447853991,2.1078487813450479,2.133938948319571,1.9730919570264065,1.7843198137229148,1.8420535681090329,2.0815124023813301,1.3495926171168444,2.2193302654254836,null,null,null,22,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_22*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_22*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.1397340999439747},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_22*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_22*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.8835621751014049},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_22*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_22*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.1710842447853991},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_22*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_22*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.1710842447853991},null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22]
[null,23,2.1972041063874603,2.1332078702790875,2.1522491782568465,1.9930755149780357,1.8034809650157204,1.8575099846629943,2.1063301443545082,1.3658292843318194,2.2460305648364396,null,null,null,23,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_23*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_23*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.1653982196759269},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_23*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_23*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.9062229186679862},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_23*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_23*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.1972041063874603},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_23*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_23*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.1972041063874603},null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23]
[null,24,2.2233239679895198,2.1585669592131262,2.1705594081941211,2.0130590729296647,1.822642116308526,1.8729664012169562,2.1311428613617496,1.3820659515467932,2.2727308642473938,null,null,null,24,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_24*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_24*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.1910605806698},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_24*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_24*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.9288836622345655},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_24*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_24*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.2233239679895198},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_24*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_24*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.2233239679895198},null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24]
[null,25,2.2494438295915811,2.1839260481471658,2.1888696381313966,2.0330426308812939,1.8418032676013318,1.8884228177709181,2.1559505637690375,1.398302618761768,2.2994311636583498,null,null,null,25,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_25*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_25*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.2167211865536909},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_25*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_25*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.9515444058011464},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_25*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_25*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.2494438295915811},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_25*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_25*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.2494438295915811},null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25]
[null,26,2.275563691193641,2.209285137081205,2.2071798680686716,2.0530261888329235,1.8609644188941372,1.9038792343248798,2.1807532619138628,1.4145392859767421,2.3261314630693044,null,null,null,26,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_26*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_26*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.2423800409457186},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_26*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_26*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.9742051493677264},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_26*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_26*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.275563691193641},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_26*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_26*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.275563691193641},null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26]
[null,27,2.3016835527957018,2.2346442260152442,2.2254900980059471,2.0730097467845527,1.880125570186943,1.9193356508788413,2.2055509661053221,1.4307759531917168,2.3528317624802599,null,null,null,27,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_27*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_27*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.268037147454069},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_27*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_27*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.9968658929343071},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_27*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_27*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.3016835527957018},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_27*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_27*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.3016835527957018},null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27]
[null,28,2.3278034143977626,2.2600033149492837,2.2438003279432217,2.0929933047361819,1.8992867214797489,1.9347920674328032,2.2303436866242139,1.4470126204066913,2.3795320618912155,null,null,null,28,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_28*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_28*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.2936925096770207},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_28*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_28*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.0195266365008875},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_28*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_28*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.3278034143977626},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_28*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_28*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.3278034143977626},null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28]
[null,29,2.3539232759998225,2.2853624038833229,2.2621105578804972,2.1129768626878112,1.9184478727725547,1.9502484839867651,2.2551314337231374,1.4632492876216654,2.4062323613021701,null,null,null,29,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_29*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_29*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.3193461312029826},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_29*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_29*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.0421873800674675},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_29*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_29*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.3539232759998225},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_29*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_29*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.3539232759998225},null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29]
[null,30,2.3800431376018834,2.3107214928173625,2.2804207878177722,2.1329604206394404,1.9376090240653601,1.9657049005407266,2.2799142176265881,1.4794859548366401,2.4329326607131261,null,null,null,30,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_30*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_30*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.3449980156105301},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_30*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_30*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.0648481236340483},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_30*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_30*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.3800431376018834},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_30*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_30*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.3800431376018834},null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30]
[null,31,2.4061629992039442,2.3360805817514017,2.2987310177550473,2.1529439785910696,1.9567701753581659,1.9811613170946885,2.3046920485310554,1.4957226220516147,2.4596329601240816,null,null,null,31,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_31*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_31*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.3706481664684329},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_31*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_31*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.0875088672006288},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_31*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_31*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.4061629992039442},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_31*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_31*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.4061629992039442},null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31]
[null,32,2.4322828608060041,2.3614396706854408,2.3170412476923228,2.1729275365426992,1.9759313266509713,1.9966177336486501,2.3294649366051146,1.5119592892665887,2.4863332595350363,null,null,null,32,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_32*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_32*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.396296587335693},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_32*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_32*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.1101696107672088},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_32*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_32*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.4322828608060041},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_32*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_32*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.4322828608060041},null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32]
[null,33,2.4584027224080649,2.3867987596194804,2.3353514776295978,2.1929110944943284,1.9950924779437771,2.0120741502026118,2.3542328919895286,1.5281959564815633,2.5130335589459918,null,null,null,33,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_33*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_33*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.4219432817615774},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_33*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_33*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.1328303543337892},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_33*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_33*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.4584027224080649},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_33*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_33*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.4584027224080649},null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33]
[null,34,2.4845225840101248,2.4121578485535196,2.3536617075668733,2.2128946524459572,2.0142536292365829,2.0275305667565737,2.3789959247973362,1.5444326236965373,2.5397338583569464,null,null,null,34,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_34*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_34*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.447588253285649},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_34*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_34*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.1554910979003692},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_34*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_34*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.4845225840101248},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_34*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_34*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.4845225840101248},null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34]
[null,35,2.5106424456121856,2.4375169374875587,2.3719719375041479,2.2328782103975868,2.0334147805293887,2.0429869833105352,2.4037540451139519,1.5606692909115121,2.566434157767902,null,null,null,35,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_35*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_35*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.4732315054378038},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_35*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_35*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.1781518414669501},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_35*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_35*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.5106424456121856},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_35*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_35*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.5106424456121856},null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35]
[null,36,2.5367623072142464,2.4628760264215983,2.3902821674414234,2.252861768349216,2.0525759318221941,2.0584433998644966,2.4285072629972584,1.5769059581264866,2.5931344571788575,null,null,null,36,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_36*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_36*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.4988730417383005},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_36*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_36*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.2008125850335305},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_36*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_36*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.5367623072142464},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_36*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_36*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.5367623072142464},null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36]
[null,37,2.5628821688163064,2.488235115355637,2.408592397378698,2.2728453263008452,2.0717370831149999,2.0738998164184586,2.4532555884776985,1.5931426253414607,2.6198347565898121,null,null,null,37,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_37*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_37*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.5245128656977935},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_37*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_37*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.2234733286001105},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_37*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_37*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.5628821688163064},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_37*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_37*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.5628821688163064},null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37]
[null,38,2.5890020304183672,2.5135942042896766,2.4269026273159735,2.2928288842524744,2.0908982344078053,2.0893562329724205,2.4779990315583724,1.6093792925564354,2.6465350560007677,null,null,null,38,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_38*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_38*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.550150980817369},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_38*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_38*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.2461340721666909},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_38*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_38*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.5890020304183672},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_38*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_38*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.5890020304183672},null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38]
[null,39,2.6151218920204271,2.5389532932237158,2.4452128572532486,2.3128124422041036,2.1100593857006111,2.1048126495263824,2.5027376022151273,1.6256159597714095,2.6732353554117223,null,null,null,39,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_39*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_39*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.5757873905885722},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_39*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_39*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.2687948157332709},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_39*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_39*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.6151218920204271},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_39*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_39*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.6151218920204271},null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39]
[null,40,2.6412417536224879,2.5643123821577554,2.463523087190524,2.3327960001557329,2.129220536993417,2.1202690660803443,2.5274713103966526,1.641852626986384,2.6999356548226778,null,null,null,40,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_40*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_40*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.6014220984934457},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_40*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_40*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.2914555592998518},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_40*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_40*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.6412417536224879},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_40*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_40*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.6412417536224879},null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40]
[null,41,2.6673616152245487,2.5896714710917945,2.4818333171277991,2.3527795581073625,2.1483816882862228,2.1357254826343057,2.5522001660245714,1.6580892942013588,2.7266359542336334,null,null,null,41,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_41*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_41*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.6270551080045568},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_41*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_41*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.3141163028664322},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_41*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_41*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.6673616152245487},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_41*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_41*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.6673616152245487},null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41]
[null,42,2.6934814768266087,2.6150305600258341,2.5001435470650741,2.3727631160589917,2.1675428395790282,2.1511818991882676,2.576924178993532,1.6743259614163328,2.7533362536445884,null,null,null,42,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_42*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_42*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.652686422585032},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_42*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_42*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.3367770464330118},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_42*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_42*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.6934814768266087},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_42*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_42*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.6934814768266087},null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42]
[null,43,2.7196013384286695,2.6403896489598733,2.5184537770023492,2.3927466740106209,2.186703990871834,2.1666383157422291,2.6016433591712995,1.6905626286313074,2.780036553055544,null,null,null,43,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_43*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_43*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.6783160456885899},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_43*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_43*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.3594377899995926},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_43*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_43*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.7196013384286695},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_43*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_43*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.7196013384286695},null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43]
[null,44,2.7457212000307303,2.6657487378939129,2.5367640069396242,2.4127302319622501,2.2058651421646394,2.182094732296191,2.6263577163988492,1.7067992958462821,2.8067368524664995,null,null,null,44,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_44*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_44*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.703943980759572},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_44*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_44*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.3820985335661735},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_44*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_44*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.7457212000307303},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_44*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_44*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.7457212000307303},null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44]
[null,45,2.7718410616327902,2.6911078268279516,2.5550742368768997,2.4327137899138793,2.2250262934574452,2.1975511488501525,2.651067260490453,1.7230359630612559,2.8334371518774542,null,null,null,45,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_45*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_45*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.7295702312329722},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_45*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_45*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.4047592771327531},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_45*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_45*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.7718410616327902},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_45*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_45*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.7718410616327902},null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45]
[null,46,2.797960923234851,2.7164669157619912,2.5733844668141748,2.4526973478655085,2.244187444750251,2.2130075654041144,2.6757720012337747,1.7392726302762307,2.8601374512884097,null,null,null,46,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_46*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_46*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.7551948005344742},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_46*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_46*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.4274200206993339},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_46*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_46*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.797960923234851},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_46*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_46*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.797960923234851},null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46]
[null,47,2.8240807848369109,2.7418260046960303,2.5916946967514503,2.4726809058171382,2.2633485960430568,2.2284639819580758,2.7004719483899584,1.7555092974912048,2.8868377506993643,null,null,null,47,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_47*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_47*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.7808176920804777},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_47*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_47*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.4500807642659139},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_47*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_47*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.8240807848369109},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_47*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_47*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.8240807848369109},null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47]
[null,48,2.8502006464389718,2.7671850936300695,2.6100049266887249,2.4926644637687674,2.2825097473358622,2.2439203985120377,2.7251671116937159,1.7717459647061793,2.9135380501103199,null,null,null,48,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_48*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_48*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.8064389092781319},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_48*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_48*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.4727415078324944},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_48*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_48*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.8502006464389718},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_48*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_48*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.8502006464389718},null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48]
[null,49,2.8763205080410326,2.7925441825641091,2.6283151566259999,2.5126480217203966,2.301670898628668,2.2593768150659996,2.7498575008534196,1.787982631921154,2.9402383495212754,null,null,null,49,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_49*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_49*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.8320584555253681},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_49*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_49*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.4954022513990752},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_49*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_49*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.8763205080410326},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_49*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_49*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.8763205080410326},null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49]
[null,{"$f":"B214+1","v":50},2.9024403696430925,2.8179032714981478,2.6466253865632754,2.5326315796720258,2.3208320499214734,2.2748332316199611,2.7745431255511899,1.8042192991361281,2.96693864893223,null,null,null,50,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_50*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_50*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.8576763342109266},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_50*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_50*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.5180629949656552},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_50*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_50*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.9024403696430925},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_50*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_50*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.9024403696430925},null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50]
[null,{"$f":"B215+1","v":51},2.9285602312451533,2.8432623604321874,2.6649356165005504,2.5526151376236546,2.3399932012142792,2.2902896481739234,2.7992239954429836,1.8204559663511026,2.9936389483431856,null,null,null,51,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_51*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_51*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.8832925487143939},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_51*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_51*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.5407237385322357},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_51*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_51*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.9285602312451533},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_51*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_51*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.9285602312451533},null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51]
[null,52,2.9546800928472137,2.868621449366227,2.6832458464378259,2.5725986955752842,2.3591543525070851,2.3057460647278849,2.8239001201586822,1.8366926335660769,3.0203392477541406,null,null,null,52,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_52*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_52*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.9089071024062276},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_52*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_52*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.5633844820988156},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_52*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_52*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.9546800928472137},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_52*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_52*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.9546800928472137},null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52]
[null,53,2.980799954449274,2.8939805383002661,2.701556076375101,2.5925822535269134,2.3783155037998909,2.3212024812818464,2.8485715093021819,1.8529293007810514,3.0470395471650957,null,null,null,53,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_53*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_53*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.9345199986477919},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_53*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_53*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.5860452256653961},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_53*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_53*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.980799954449274},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_53*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_53*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.980799954449274},null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53]
[null,54,3.0069198160513348,2.9193396272343057,2.719866306312376,2.6125658114785431,2.3974766550926967,2.3366588978358083,2.8732381724514782,1.869165967996026,3.0737398465760517,null,null,null,54,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_54*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_54*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.9601312407913847},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_54*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_54*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.608705969231977},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_54*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_54*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.0069198160513348},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_54*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_54*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.0069198160513348},null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54]
[null,55,3.0330396776533948,2.9446987161683449,2.7381765362496511,2.6325493694301723,2.4166378063855021,2.3521153143897697,2.8979001191587548,1.885402635211,3.1004401459870063,null,null,null,55,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_55*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_55*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.9857408321802708},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_55*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_55*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.6313667127985565},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_55*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_55*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.0330396776533948},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_55*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_55*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.0330396776533948},null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55]
[null,56,3.0591595392554556,2.970057805102384,2.7564867661869261,2.652532927381801,2.4357989576783079,2.3675717309437316,2.9225573589504701,1.9016393024259748,3.1271404453979619,null,null,null,56,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_56*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_56*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.0113487761487105},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_56*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_56*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.6540274563651374},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_56*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_56*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.0591595392554556},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_56*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_56*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.0591595392554556},null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56]
[null,57,3.085279400857516,2.9954168940364236,2.7747969961242012,2.6725164853334302,2.4549601089711133,2.3830281474976935,2.9472099013274446,1.9178759696409491,3.153840744808917,null,null,null,57,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_57*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_57*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.0369550760219908},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_57*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_57*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.6766881999317174},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_57*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_57*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.085279400857516},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_57*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_57*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.085279400857516},null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57]
[null,58,3.1113992624595763,3.0207759829704623,2.7931072260614767,2.6925000432850594,2.4741212602639191,2.398484564051655,2.9718577557649444,1.9341126368559234,3.180541044219872,null,null,null,58,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_58*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_58*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.0625597351164551},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_58*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_58*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.6993489434982978},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_58*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_58*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1113992624595763},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_58*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_58*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1113992624595763},null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58]
[null,59,3.1375191240616371,3.0461350719045019,2.8114174559987517,2.7124836012366891,2.4932824115567249,2.4139409806056169,2.9965009317127724,1.9503493040708979,3.2072413436308276,null,null,null,59,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_59*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_59*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.0881627567395347},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_59*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_59*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.7220096870648782},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_59*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_59*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1375191240616371},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_59*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_59*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1375191240616371},null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59]
[null,60,3.1636389856636975,3.0714941608385411,2.8297276859360267,2.7324671591883187,2.5124435628495307,2.4293973971595788,3.0211394385953474,1.9665859712858724,3.2339416430417827,null,null,null,60,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_60*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_14.6_60*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.113764144189775},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_60*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_14.6_60*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.7446704306314587},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_60*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_14.6_60*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1636389856636975},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_14.6_60*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_14.6_60*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1636389856636975},null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60]
[]
[]
[]
[]
[]
[]
["Busstørrelse","Hastighed (km/t)","Euro 6","EEV","Euro 5","Euro 4","Euro 3","Euro 2","Biodiesel","Ethanol","Gas",null,null,"Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol","Busstørrelse","Hastighed i km/t","Biodiesel","Ethanol","Biodiesel","Ethanol"]
["18 meter",10,1.1292827794884857,1.0963910480470733,1.1636724588182203,1.0536850479123796,0.94492784399937946,1.0070505833200474,1.0840893825977516,0.70198644087415252,1.1543777984489678,null,null,"18 meter",10,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_10*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_10*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.1134650905767287},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_10*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_10*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":0.97972906097346912},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_10*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_10*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.1292827794884857},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_10*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_10*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.1292827794884857},"18 meter",10,null,null,null,null,"18 meter",10,null,null,null,null,"18 meter",10,null,null,null,null,"18 meter",10,null,null,null,null,"18 meter",10,null,null,null,null,"18 meter",10,null,null,null,null,"18 meter",10,null,null,null,null,"18 meter",10,null,null,null,null,"18 meter",10,null,null,null,null,"18 meter",10,null,null,null,null,"18 meter",10,null,null,null,null,"18 meter",10,null,null,null,null,"18 meter",10,null,null,null,null,"18 meter",10,null,null,null,null,"18 meter",10,null,null,null,null,"18 meter",10,null,null,null,null,"18 meter",10,null,null,null,null,"18 meter",10,null,null,null,null,"18 meter",10,null,null,null,null,"18 meter",10,null,null,null,null,"18 meter",10,null,null,null,null,"18 meter",10,null,null,null,null,"18 meter",10,null,null,null,null,"18 meter",10]
[null,{"$f":"B233+1","v":11},1.1451613222298844,1.1118071089610528,1.1748034430896273,1.0658332661493066,0.95657611244783158,1.0164467039664746,1.0992135075909351,0.71185688422789917,1.1706091955315445,null,null,null,11,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_11*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_11*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.1290795871062522},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_11*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_11*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":0.9935047689291896},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_11*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_11*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.1451613222298844},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_11*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_11*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.1451613222298844},null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11,null,null,null,null,null,11]
[null,{"$f":"B234+1","v":12},1.161039864971283,1.1272231698750321,1.1859344273610342,1.0779814843862339,0.96822438089628393,1.0258428246129021,1.1143345008615657,0.72172732758164571,1.1868405926141212,null,null,null,12,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_12*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_12*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.144692987532882},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_12*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_12*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.00728047688491},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_12*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_12*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.161039864971283},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_12*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_12*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.161039864971283},null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12,null,null,null,null,null,12]
[null,13,1.1769184077126815,1.1426392307890114,1.1970654116324413,1.0901297026231609,0.97987264934473628,1.0352389452593291,1.1294523689238145,0.73159777093539213,1.2030719896966979,null,null,null,13,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_13*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_13*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.1603052941365781},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_13*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_13*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.0210561848406301},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_13*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_13*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.1769184077126815},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_13*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_13*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.1769184077126815},null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13,null,null,null,null,null,13]
[null,14,1.1927969504540803,1.1580552917029905,1.2081963959038482,1.1022779208600879,0.99152091779318852,1.0446350659057566,1.1445671182737982,0.74146821428913878,1.2193033867792749,null,null,null,14,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_14*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_14*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.1759165091909816},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_14*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_14*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.0348318927963507},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_14*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_14*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.1927969504540803},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_14*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_14*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.1927969504540803},null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14,null,null,null,null,null,14]
[null,15,1.2086754931954793,1.17347135261697,1.2193273801752551,1.1144261390970152,1.0031691862416408,1.0540311865521839,1.1596787553896419,0.75133865764288554,1.235534783861852,null,null,null,15,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_15*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_15*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.1915266349634361},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_15*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_15*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.0486076007520715},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_15*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_15*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.2086754931954793},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_15*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_15*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.2086754931954793},null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15,null,null,null,null,null,15]
[null,16,1.2245540359368776,1.1888874135309493,1.230458364446662,1.1265743573339422,1.0148174546900932,1.0634273071986109,1.1747872867315421,0.76120910099663186,1.2517661809444285,null,null,null,16,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_16*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_16*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.2071356737150101},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_16*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_16*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.0623833087077916},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_16*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_16*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.2245540359368776},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_16*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_16*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.2245540359368776},null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16,null,null,null,null,null,16]
[null,17,1.2404325786782764,1.2043034744449286,1.2415893487180691,1.1387225755708692,1.0264657231385454,1.0728234278450384,1.1898927187418271,0.77107954435037851,1.2679975780270054,null,null,null,17,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_17*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_17*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.222743627700519},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_17*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_17*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.0761590166635122},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_17*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_17*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.2404325786782764},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_17*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_17*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.2404325786782764},null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17,null,null,null,null,null,17]
[null,18,1.2563111214196752,1.2197195353589079,1.2527203329894758,1.1508707938077962,1.0381139915869977,1.0822195484914656,1.2049950578450206,0.78094998770412505,1.2842289751095823,null,null,null,18,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_18*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_18*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.2383504991685461},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_18*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_18*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.0899347246192326},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_18*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_18*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.2563111214196752},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_18*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_18*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.2563111214196752},null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18,null,null,null,null,null,18]
[null,19,1.2721896641610737,1.2351355962728892,1.263851317260883,1.1630190120447235,1.0497622600354501,1.0916156691378929,1.2200943104479016,0.79082043105787159,1.300460372192159,null,null,null,19,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_19*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_19*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.2539562903614634},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_19*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_19*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.1037104325749529},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_19*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_19*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.2721896641610737},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_19*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_19*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.2721896641610737},null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19,null,null,null,null,null,19]
[null,20,1.2880682069024725,1.2505516571868664,1.2749823015322899,1.1751672302816505,1.0614105284839022,1.1010117897843201,1.2351904829395672,0.80069087441161824,1.316691769274736,null,null,null,20,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_20*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_20*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.2695610035154556},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_20*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_20*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.1174861405306735},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_20*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_20*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.2880682069024725},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_20*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_20*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.2880682069024725},null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20,null,null,null,null,null,20]
[null,21,1.303946749643871,1.2659677181008457,1.2861132858036968,1.1873154485185777,1.0730587969323546,1.1104079104307474,1.2502835816914915,0.81056131776536466,1.3329231663573127,null,null,null,21,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_21*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_21*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.2851646408605382},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_21*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_21*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.1312618484863939},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_21*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_21*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.303946749643871},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_21*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_21*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.303946749643871},null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21,null,null,null,null,null,21]
[null,22,1.3198252923852698,1.281383779014825,1.2972442700751037,1.1994636667555048,1.0847070653808071,1.1198040310771749,1.2653736130575874,0.82043176111911131,1.3491545634398896,null,null,null,22,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_22*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_22*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.3007672046205809},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_22*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_22*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.1450375564421142},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_22*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_22*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.3198252923852698},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_22*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_22*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.3198252923852698},null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22,null,null,null,null,null,22]
[null,23,1.3357038351266688,1.2967998399288045,1.3083752543465106,1.2116118849924318,1.0963553338292593,1.1292001517236019,1.2804605833742688,0.83030220447285807,1.3653859605224665,null,null,null,23,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_23*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_23*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.3163686970133288},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_23*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_23*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.1588132643978351},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_23*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_23*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.3357038351266688},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_23*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_23*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.3357038351266688},null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23,null,null,null,null,null,23]
[null,24,1.3515823778680671,1.3122159008427836,1.3195062386179175,1.223760103229359,1.1080036022777116,1.1385962723700294,1.2955444989605072,0.84017264782660439,1.381617357605043,null,null,null,24,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_24*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_24*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.3319691202504211},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_24*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_24*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.1725889723535552},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_24*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_24*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.3515823778680671},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_24*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_24*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.3515823778680671},null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24,null,null,null,null,null,24]
[null,25,1.3674609206094659,1.3276319617567631,1.3306372228893244,1.235908321466286,1.1196518707261638,1.1479923930164566,1.3106253661178948,0.85004309118035104,1.3978487546876199,null,null,null,25,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_25*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_25*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.3475684765374161},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_25*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_25*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.1863646803092758},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_25*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_25*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.3674609206094659},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_25*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_25*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.3674609206094659},null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25,null,null,null,null,null,25]
[null,26,1.3833394633508644,1.3430480226707422,1.3417682071607315,1.2480565397032133,1.131300139174616,1.1573885136628839,1.3257031911307025,0.85991353453409747,1.4140801517701966,null,null,null,26,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_26*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_26*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.3631667680738078},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_26*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_26*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.2001403882649959},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_26*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_26*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.3833394633508644},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_26*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_26*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.3833394633508644},null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26,null,null,null,null,null,26]
[null,27,1.3992180060922632,1.3584640835847215,1.3528991914321384,1.2602047579401403,1.1429484076230685,1.1667846343093111,1.3407779802659399,0.86978397788784412,1.4303115488527736,null,null,null,27,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_27*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_27*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.3787639970530501},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_27*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_27*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.2139160962207165},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_27*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_27*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.3992180060922632},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_27*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_27*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.3992180060922632},null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27,null,null,null,null,null,27]
[null,28,1.4150965488336622,1.373880144498701,1.3640301757035453,1.2723529761770676,1.1545966760715207,1.1761807549557384,1.3558497397734144,0.87965442124159088,1.4465429459353507,null,null,null,28,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_28*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_28*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.3943601656625755},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_28*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_28*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.2276918041764373},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_28*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_28*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.4150965488336622},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_28*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_28*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.4150965488336622},null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28,null,null,null,null,null,28]
[null,29,1.4309750915750605,1.3892962054126803,1.3751611599749523,1.2845011944139946,1.1662449445199732,1.1855768756021658,1.3709184758857906,0.88952486459533719,1.4627743430179272,null,null,null,29,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_29*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_29*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.4099552760838159},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_29*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_29*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.2414675121321572},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_29*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_29*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.4309750915750605},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_29*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_29*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.4309750915750605},null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29,null,null,null,null,null,29]
[null,30,1.4468536343164593,1.4047122663266596,1.3862921442463592,1.2966494126509216,1.1778932129684252,1.1949729962485929,1.3859841948186484,0.89939530794908384,1.4790057401005041,null,null,null,30,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_30*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_30*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.4255493304922253},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_30*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_30*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.2552432200878778},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_30*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_30*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.4468536343164593},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_30*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_30*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.4468536343164593},null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30,null,null,null,null,null,30]
[null,31,1.4627321770578583,1.4201283272406391,1.3974231285177661,1.3087976308878486,1.1895414814168777,1.2043691168950201,1.4010469027705428,0.9092657513028306,1.4952371371830813,null,null,null,31,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_31*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_31*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.4411423310572979},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_31*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_31*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.2690189280435986},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_31*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_31*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.4627321770578583},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_31*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_31*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.4627321770578583},null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31,null,null,null,null,null,31]
[null,32,1.4786107197992566,1.4355443881546182,1.4085541127891732,1.3209458491247759,1.2011897498653299,1.2137652375414476,1.4161066059230589,0.91913619465657692,1.5114685342656577,null,null,null,32,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_32*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_32*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.4567342799425873},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_32*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_32*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.2827946359993188},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_32*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_32*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.4786107197992566},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_32*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_32*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.4786107197992566},null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32,null,null,null,null,null,32]
[null,33,1.4944892625406554,1.4509604490685974,1.4196850970605801,1.3330940673617029,1.2128380183137821,1.2231613581878746,1.431163310440875,0.92900663801032357,1.5276999313482347,null,null,null,33,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_33*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_33*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.4723251793057321},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_33*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_33*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.2965703439550391},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_33*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_33*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.4944892625406554},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_33*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_33*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.4944892625406554},null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33,null,null,null,null,null,33]
[null,34,1.5103678052820539,1.4663765099825767,1.430816081331987,1.3452422855986299,1.2244862867622346,1.2325574788343021,1.4462170224718152,0.93887708136407,1.5439313284308114,null,null,null,34,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_34*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_34*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.4879150312984704},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_34*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_34*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.3103460519107597},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_34*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_34*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.5103678052820539},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_34*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_34*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.5103678052820539},null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34,null,null,null,null,null,34]
[null,35,1.5262463480234527,1.481792570896556,1.4419470656033939,1.3573905038355571,1.2361345552106868,1.2419535994807294,1.4612677481469107,0.94874752471781665,1.5601627255133881,null,null,null,35,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_35*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_35*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.503503838066663},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_35*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_35*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.3241217598664801},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_35*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_35*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.5262463480234527},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_35*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_35*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.5262463480234527},null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35,null,null,null,null,null,35]
[null,36,1.5421248907648517,1.4972086318105355,1.4530780498748008,1.3695387220724842,1.2477828236591391,1.2513497201271566,1.4763154935804559,0.95861796807156341,1.5763941225959652,null,null,null,36,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_36*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_36*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.5190916017503131},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_36*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_36*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.3378974678222009},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_36*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_36*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.5421248907648517},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_36*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_36*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.5421248907648517},null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36,null,null,null,null,null,36]
[null,37,1.55800343350625,1.5126246927245146,1.4642090341462077,1.3816869403094112,1.2594310921075915,1.2607458407735839,1.4913602648700637,0.96848841142530973,1.5926255196785417,null,null,null,37,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_37*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_37*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.5346783244835849},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_37*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_37*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.351673175777921},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_37*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_37*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.55800343350625},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_37*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_37*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.55800343350625},null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37,null,null,null,null,null,37]
[null,38,1.5738819762476488,1.5280407536384941,1.4753400184176146,1.3938351585463382,1.2710793605560435,1.2701419614200111,1.5064020680967261,0.97835885477905637,1.6088569167611186,null,null,null,38,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_38*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_38*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.5502640083948258},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_38*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_38*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.3654488837336414},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_38*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_38*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.5738819762476488},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_38*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_38*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.5738819762476488},null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38,null,null,null,null,null,38]
[null,39,1.5897605189890474,1.5434568145524732,1.4864710026890218,1.4059833767832655,1.282727629004496,1.2795380820664386,1.5214409093248669,0.98822929813280291,1.6250883138436953,null,null,null,39,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_39*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_39*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.565848655606584},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_39*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_39*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.3792245916893617},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_39*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_39*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.5897605189890474},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_39*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_39*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.5897605189890474},null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39,null,null,null,null,null,39]
[null,40,1.6056390617304461,1.5588728754664525,1.4976019869604287,1.4181315950201925,1.2943758974529482,1.2889342027128659,1.5364767946024001,0.99809974148654945,1.6413197109262723,null,null,null,40,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_40*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_40*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.5814322682356301},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_40*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_40*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.3930002996450823},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_40*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_40*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.6056390617304461},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_40*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_40*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.6056390617304461},null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40,null,null,null,null,null,40]
[null,41,1.6215176044718451,1.574288936380432,1.5087329712318356,1.4302798132571197,1.3060241659014007,1.2983303233592931,1.5515097299607872,1.0079701848402962,1.6575511080088494,null,null,null,41,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_41*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_41*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.5970148483929749},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_41*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_41*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.4067760076008031},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_41*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_41*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.6215176044718451},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_41*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_41*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.6215176044718451},null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41,null,null,null,null,null,41]
[null,42,1.6373961472132434,1.5897049972944113,1.5198639555032425,1.4424280314940467,1.3176724343498529,1.3077264440057204,1.5665397214150896,1.0178406281940426,1.6737825050914259,null,null,null,42,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_42*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_42*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.6125963981838896},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_42*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_42*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.420551715556523},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_42*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_42*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.6373961472132434},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_42*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_42*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.6373961472132434},null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42,null,null,null,null,null,42]
[null,43,1.6532746899546422,1.6051210582083906,1.5309949397746494,1.4545762497309738,1.3293207027983052,1.3171225646521476,1.5815667749640279,1.0277110715477893,1.6900139021740028,null,null,null,43,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_43*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_43*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.6281769197079274},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_43*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_43*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.4343274235122438},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_43*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_43*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.6532746899546422},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_43*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_43*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.6532746899546422},null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43,null,null,null,null,null,43]
[null,44,1.6691532326960412,1.6205371191223701,1.5421259240460563,1.4667244679679008,1.3409689712467574,1.3265186852985749,1.5965908965900353,1.0375815149015359,1.70624529925658,null,null,null,44,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_44*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_44*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.6437564150589392},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_44*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_44*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.4481031314679644},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_44*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_44*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.6691532326960412},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_44*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_44*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.6691532326960412},null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44,null,null,null,null,null,44]
[null,45,1.6850317754374395,1.6359531800363489,1.5532569083174634,1.4788726862048278,1.3526172396952099,1.3359148059450021,1.6116120922593133,1.0474519582552824,1.7224766963391565,null,null,null,45,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_45*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_45*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.6593348863250954},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_45*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_45*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.4618788394236846},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_45*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_45*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.6850317754374395},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_45*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_45*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.6850317754374395},null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45,null,null,null,null,null,45]
[null,46,1.7009103181788383,1.6513692409503284,1.5643878925888703,1.4910209044417551,1.3642655081436621,1.3453109265914296,1.6266303679218865,1.057322401609029,1.7387080934217334,null,null,null,46,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_46*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_46*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.6749123355889051},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_46*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_46*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.4756545473794049},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_46*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_46*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.7009103181788383},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_46*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_46*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.7009103181788383},null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46,null,null,null,null,null,46]
[null,47,1.7167888609202369,1.6667853018643077,1.5755188768602775,1.5031691226786823,1.3759137765921146,1.3547070472378566,1.6416457295116589,1.0671928449627754,1.7549394905043099,null,null,null,47,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_47*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_47*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.6904887649272347},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_47*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_47*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.4894302553351253},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_47*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_47*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.7167888609202369},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_47*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_47*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.7167888609202369},null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47,null,null,null,null,null,47]
[null,48,1.7326674036616356,1.682201362778287,1.5866498611316842,1.5153173409156093,1.3875620450405666,1.3641031678842839,1.6566581829464659,1.0770632883165221,1.7711708875868868,null,null,null,48,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_48*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_48*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.7060641764113265},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_48*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_48*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.5032059632908461},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_48*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_48*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.7326674036616356},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_48*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_48*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.7326674036616356},null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48,null,null,null,null,null,48]
[null,49,1.7485459464030346,1.6976174236922665,1.5977808454030911,1.5274655591525363,1.399210313489019,1.3734992885307113,1.6716677341281305,1.0869337316702687,1.7874022846694639,null,null,null,49,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_49*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_49*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.7216385721068184},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_49*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_49*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.5169816712465667},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_49*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_49*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.7485459464030346},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_49*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_49*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.7485459464030346},null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49,null,null,null,null,null,49]
[null,{"$f":"B272+1","v":50},1.764424489144433,1.7130334846062456,1.608911829674498,1.5396137773894634,1.4108585819374713,1.3828954091771384,1.6866743889425171,1.0968041750240152,1.8036336817520404,null,null,null,50,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_50*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_50*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.7372119540737625},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_50*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_50*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.5307573792022868},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_50*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_50*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.764424489144433},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_50*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_50*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.764424489144433},null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50,null,null,null,null,null,50]
[null,{"$f":"B273+1","v":51},1.7803030318858317,1.7284495455202249,1.6200428139459049,1.5517619956263904,1.4225068503859235,1.3922915298235661,1.7016781532595848,1.1066746183777618,1.8198650788346173,null,null,null,51,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_51*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_51*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.7527843243666454},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_51*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_51*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.5445330871580074},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_51*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_51*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.7803030318858317},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_51*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_51*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.7803030318858317},null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51,null,null,null,null,null,51]
[null,52,1.7961815746272305,1.7438656064342042,1.631173798217312,1.5639102138633176,1.434155118834376,1.4016876504699931,1.716679032933442,1.1165450617315085,1.8360964759171943,null,null,null,52,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_52*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_52*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.7683556850344044},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_52*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_52*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.5583087951137278},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_52*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_52*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.7961815746272305},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_52*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_52*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.7961815746272305},null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52,null,null,null,null,null,52]
[null,53,1.812060117368629,1.7592816673481835,1.6423047824887189,1.5760584321002447,1.4458033872828282,1.4110837711164204,1.7316770338023988,1.1264155050852549,1.852327872999771,null,null,null,53,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_53*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_53*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.7839260381204485},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_53*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_53*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.5720845030694481},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_53*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_53*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.812060117368629},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_53*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_53*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.812060117368629},null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53,null,null,null,null,null,53]
[null,54,1.8279386601100278,1.774697728262163,1.6534357667601258,1.5882066503371719,1.4574516557312807,1.4204798917628478,1.7466721616890217,1.1362859484390015,1.8685592700823479,null,null,null,54,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_54*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_54*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.7994953856626756},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_54*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_54*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.5858602110251685},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_54*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_54*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.8279386601100278},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_54*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_54*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.8279386601100278},null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54,null,null,null,null,null,54]
[null,55,1.8438172028514264,1.7901137891761423,1.6645667510315327,1.6003548685740989,1.4690999241797329,1.4298760124092749,1.7616644224001847,1.146156391792748,1.8847906671649246,null,null,null,55,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_55*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_55*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.8150637296934917},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_55*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_55*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.5996359189808889},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_55*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_55*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.8438172028514264},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_55*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_55*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.8438172028514264},null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55,null,null,null,null,null,55]
[null,56,1.8596957455928251,1.8055298500901216,1.6756977353029396,1.6125030868110259,1.4807481926281849,1.4392721330557023,1.7766538217271239,1.1560268351464946,1.9010220642475015,null,null,null,56,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_56*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_56*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.8306310722398298},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_56*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_56*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.6134116269366094},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_56*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_56*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.8596957455928251},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_56*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_56*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.8596957455928251},null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56,null,null,null,null,null,56]
[null,57,1.8755742883342239,1.8209459110041009,1.6868287195743465,1.624651305047953,1.4923964610766374,1.4486682537021296,1.7916403654454893,1.1658972785002413,1.9172534613300785,null,null,null,57,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_57*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_57*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.8461974153231666},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_57*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_57*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.62718733489233},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_57*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_57*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.8755742883342239},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_57*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_57*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.8755742883342239},null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57,null,null,null,null,null,57]
[null,58,1.8914528310756225,1.8363619719180799,1.6979597038457537,1.63679952328488,1.5040447295250896,1.4580643743485568,1.8066240593153962,1.1757677218539877,1.9334848584126552,null,null,null,58,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_58*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_58*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.8617627609595431},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_58*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_58*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.6409630428480502},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_58*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_58*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.8914528310756225},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_58*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_58*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.8914528310756225},null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58,null,null,null,null,null,58]
[null,59,1.9073313738170212,1.8517780328320594,1.7090906881171606,1.6489477415218072,1.5156929979735421,1.4674604949949841,1.821604909081481,1.1856381652077344,1.9497162554952321,null,null,null,59,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_59*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_59*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.8773271111595822},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_59*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_59*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.654738750803771},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_59*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_59*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.9073313738170212},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_59*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_59*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.9073313738170212},null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59,null,null,null,null,null,59]
[null,60,1.9232099165584198,1.8671940937460387,1.7202216723885675,1.6610959597587345,1.5273412664219945,1.4768566156414114,1.8365829204729485,1.1955086085614808,1.9659476525778086,null,null,null,60,{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_60*(1-'Vurdering af miljøgevinst'!$B$13)+Biodiesel_18_60*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.8928904679285048},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_60*(1-'Vurdering af miljøgevinst'!$B$13)+Ethanol_18_60*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.6685144587594911},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_60*(1-'Vurdering af miljøgevinst'!$F$13)+Biodiesel_18_60*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.9232099165584198},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Euro6_18_60*(1-'Vurdering af miljøgevinst'!$F$13)+Ethanol_18_60*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.9232099165584198},null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60,null,null,null,null,null,60]
[]
[]
[]
[]
[]
[]
[]
[]
["10 km/t"]
["11 km/t"]
["12 km/t"]
["13 km/t"]
["14 km/t"]
["15 km/t"]
["16 km/t"]
["17 km/t"]
["18 km/t"]
["19 km/t"]
["20 km/t"]
["21 km/t"]
["22 km/t"]
["23 km/t"]
["24 km/t"]
["25 km/t"]
["26 km/t"]
["27 km/t"]
["28 km/t"]
["29 km/t"]
["30 km/t"]
["31 km/t"]
["32 km/t"]
["33 km/t"]
["34 km/t"]
["35 km/t"]
["36 km/t"]
["37 km/t"]
["38 km/t"]
["39 km/t"]
["40 km/t"]
["41 km/t"]
["42 km/t"]
["43 km/t"]
["44 km/t"]
["45 km/t"]
["46 km/t"]
["47 km/t"]
["48 km/t"]
["49 km/t"]
["50 km/t"]
["51 km/t"]
["52 km/t"]
["53 km/t"]
["54 km/t"]
["55 km/t"]
["56 km/t"]
["57 km/t"]
["58 km/t"]
["59 km/t"]
["60 km/t"]

{"sheet":"Diverse","index":6,"n_rows":177,"n_cols":41,"rows_kept":177,"cut":false,"hidden":true,"merged":[[0,37,0,40],[1,37,1,38],[1,39,1,40],[0,25,0,28],[1,25,1,26],[1,27,1,28],[0,31,0,34],[1,31,1,32],[1,33,1,34],[1,13,1,14],[1,15,1,16],[0,7,0,10],[0,13,0,16],[0,19,0,22],[1,19,1,20],[1,21,1,22],[0,1,0,4],[1,1,1,2],[1,3,1,4],[1,7,1,8],[1,9,1,10]]}
[null,"Energiindhold ved blandingsforhold",null,null,null,"Euro 6",null,"Emissioner ved blandingsforhold",null,null,null,"EEV",null,"Emissioner ved blandingsforhold",null,null,null,"Euro 5",null,"Emissioner ved blandingsforhold",null,null,null,"Euro 4",null,"Emissioner ved blandingsforhold",null,null,null,"Euro 3",null,"Emissioner ved blandingsforhold",null,null,null,"Euro 2",null,"Emissioner ved blandingsforhold"]
[null,"Tiltag",null,"Reference",null,null,null,"Tiltag",null,"Reference",null,null,null,"Tiltag",null,"Reference",null,null,null,"Tiltag",null,"Reference",null,null,null,"Tiltag",null,"Reference",null,null,null,"Tiltag",null,"Reference",null,null,null,"Tiltag",null,"Reference"]
[null,"Biodiesel","Ethanol","Biodiesel","Ethanol",null,null,"Biodiesel","Ethanol","Biodiesel","Ethanol",null,null,"Biodiesel","Ethanol","Biodiesel","Ethanol",null,null,"Biodiesel","Ethanol","Biodiesel","Ethanol",null,null,"Biodiesel","Ethanol","Biodiesel","Ethanol",null,null,"Biodiesel","Ethanol","Biodiesel","Ethanol",null,null,"Biodiesel","Ethanol","Biodiesel","Ethanol"]
["Rute 1",{"$f":"IF('Vurdering af miljøgevinst'!A5=\"Rute 1\",Brændstoftyper!$B$14*(1-'Vurdering af miljøgevinst'!B13)+Brændstoftyper!$C$14*'Vurdering af miljøgevinst'!B13,\"IR\")","v":33.934449999999998},{"$f":"IF('Vurdering af miljøgevinst'!A5=\"Rute 1\",Brændstoftyper!$B$14*(1-'Vurdering af miljøgevinst'!B13)+Brændstoftyper!$F$14*'Vurdering af miljøgevinst'!B13,\"IR\")","v":30.564999999999998},{"$f":"IF('Vurdering af miljøgevinst'!A5=\"Rute 1\",Brændstoftyper!$B$14*(1-'Vurdering af miljøgevinst'!F13)+Brændstoftyper!$C$14*'Vurdering af miljøgevinst'!F13,\"IR\")","v":35.5},{"$f":"IF('Vurdering af miljøgevinst'!A5=\"Rute 1\",Brændstoftyper!$B$14*(1-'Vurdering af miljøgevinst'!F13)+Brændstoftyper!$F$14*'Vurdering af miljøgevinst'!F13,\"IR\")","v":35.5},"Rute 1","Kuldioxid (CO2) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B23*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!C23*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1707.55},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B23*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!F23*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1707.55},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B23*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!C23*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2627},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B23*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!F23*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2627},"Rute 1","Kuldioxid (CO2) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B32*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!C32*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1707.55},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B32*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!F32*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1707.55},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B32*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!C32*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2627},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B32*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!F32*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2627},"Rute 1","Kuldioxid (CO2) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B41*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$C41*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1707.55},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B41*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$F41*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1707.55},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B41*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$C41*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2627},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B41*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$F41*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2627},"Rute 1","Kuldioxid (CO2) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B50*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$C50*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1707.55},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B50*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$F50*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1707.55},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B50*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$C50*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2627},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B50*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$F50*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2627},"Rute 1","Kuldioxid (CO2) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B59*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$C59*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1707.55},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B59*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$F59*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1707.55},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B59*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$C59*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2627},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B59*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$F59*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2627},"Rute 1","Kuldioxid (CO2) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B68*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$C68*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1707.55},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B68*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$F68*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1707.55},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B68*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$C68*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2627},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B68*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$F68*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2627}]
[null,null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B24*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!C24*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.267774225E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B24*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!F24*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.44586E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B24*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!C24*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.7750000000000002E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B24*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!F24*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.7750000000000002E-2},null,"Svovldioxid (SO2) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B33*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!C33*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.267774225E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B33*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!F33*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.44586E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B33*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!C33*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.7750000000000002E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B33*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!F33*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.7750000000000002E-2},null,"Svovldioxid (SO2) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B42*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$C42*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.267774225E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B42*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$F42*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.44586E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B42*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$C42*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.7750000000000002E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B42*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$F42*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.7750000000000002E-2},null,"Svovldioxid (SO2) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B51*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$C51*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.267774225E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B51*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$F51*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.44586E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B51*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$C51*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.7750000000000002E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B51*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$F51*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.7750000000000002E-2},null,"Svovldioxid (SO2) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B60*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$C60*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.267774225E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B60*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$F60*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.44586E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B60*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$C60*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.7750000000000002E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B60*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$F60*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.7750000000000002E-2},null,"Svovldioxid (SO2) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B69*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$C69*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.267774225E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B69*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$F69*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.44586E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B69*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$C69*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.7750000000000002E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B69*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$F69*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.7750000000000002E-2}]
[null,null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B25*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!C25*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":0.79180383333333326},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B25*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!F25*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":0.66642076666666661},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B25*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!C25*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":0.82833333333333337},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B25*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!F25*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":0.82833333333333337},null,"Kvælstofilter (NOx) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B34*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!C34*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.9590191666666668},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B34*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!F34*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.8200874333333337},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B34*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!C34*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.1416666666666666},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B34*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!F34*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.1416666666666666},null,"Kvælstofilter (NOx) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B43*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$C43*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.9590191666666668},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B43*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$F43*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.8200874333333337},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B43*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$C43*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.1416666666666666},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B43*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$F43*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.1416666666666666},null,"Kvælstofilter (NOx) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B52*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$C52*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":6.9282835416666657},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B52*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$F52*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.8391499333333332},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B52*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$C52*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":7.2479166666666668},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B52*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$F52*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":7.2479166666666668},null,"Kvælstofilter (NOx) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B61*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$C61*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":9.8975479166666673},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B61*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$F61*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":6.8582124333333336},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B61*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$C61*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":10.354166666666666},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B61*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$F61*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":10.354166666666666},null,"Kvælstofilter (NOx) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B70*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$C70*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":13.856567083333331},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B70*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$F70*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":9.5502957666666664},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B70*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$C70*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":14.495833333333334},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B70*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$F70*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":14.495833333333334}]
[null,null,null,null,null,null,"Kulilte (CO) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B26*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!C26*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.9692643749999998},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B26*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!F26*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.0190625},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B26*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!C26*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1062499999999997},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B26*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!F26*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1062499999999997},null,"Kulilte (CO) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B35*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!C35*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.9692643749999998},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B35*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!F35*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.0190625},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B35*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!C35*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1062499999999997},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B35*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!F35*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1062499999999997},null,"Kulilte (CO) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B44*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$C44*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.9692643749999998},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B44*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$F44*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.0190625},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B44*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$C44*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1062499999999997},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B44*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$F44*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1062499999999997},null,"Kulilte (CO) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B53*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$C53*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.9692643749999998},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B53*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$F53*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.0190625},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B53*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$C53*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1062499999999997},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B53*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$F53*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":3.1062499999999997},null,"Kulilte (CO) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B62*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$C62*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":4.156970125},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B62*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$F62*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.8266875000000002},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B62*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$C62*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.3487499999999999},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B62*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$F62*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.3487499999999999},null,"Kulilte (CO) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B71*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$C71*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":7.9180383333333335},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B71*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$F71*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":5.3841666666666672},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B71*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$C71*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":8.2833333333333332},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B71*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$F71*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":8.2833333333333332}]
[null,null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B27*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!C27*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":0.25733624583333337},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B27*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!F27*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":0.1749854166666667},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B27*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!C27*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":0.26920833333333338},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B27*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!F27*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":0.26920833333333338},null,"Kulbrinte (HC) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B36*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!C36*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":0.49487739583333334},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B36*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!F36*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":0.3365104166666667},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B36*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!C36*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":0.51770833333333333},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B36*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!F36*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":0.51770833333333333},null,"Kulbrinte (HC) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B45*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$C45*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":0.91057440833333325},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B45*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$F45*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":0.61917916666666661},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B45*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$C45*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":0.95258333333333323},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B45*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$F45*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":0.95258333333333323},null,"Kulbrinte (HC) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B54*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$C54*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":0.91057440833333325},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B54*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$F54*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":0.61917916666666661},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B54*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$C54*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":0.95258333333333323},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B54*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$F54*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":0.95258333333333323},null,"Kulbrinte (HC) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B63*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$C63*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.3064763250000002},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B63*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$F63*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":0.88838750000000011},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B63*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$C63*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.3667500000000001},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B63*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$F63*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":1.3667500000000001},null,"Kulbrinte (HC) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B72*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$C72*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.177460541666667},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B72*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$F72*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.4806458333333337},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B72*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$C72*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.277916666666667},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B72*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$F72*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.277916666666667}]
[null,null,null,null,null,null,"Partikler (PM) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B28*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!C28*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.9795095833333335E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B28*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!F28*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":1.3460416666666669E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B28*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!C28*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.0708333333333336E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B28*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!F28*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":2.0708333333333336E-2},null,"Partikler (PM) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B37*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!C37*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.959019166666667E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B37*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!F37*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.6920833333333338E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B37*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!C37*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.1416666666666671E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!B37*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!F37*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.1416666666666671E-2},null,"Partikler (PM) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B46*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$C46*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.959019166666667E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B46*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$F46*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.6920833333333338E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B46*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$C46*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.1416666666666671E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B46*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$F46*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.1416666666666671E-2},null,"Partikler (PM) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B55*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$C55*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":3.959019166666667E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B55*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$F55*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":2.6920833333333338E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B55*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$C55*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.1416666666666671E-2},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B55*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$F55*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":4.1416666666666671E-2},null,"Partikler (PM) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B64*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$C64*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":0.19795095833333332},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B64*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$F64*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":0.13460416666666666},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B64*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$C64*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":0.20708333333333334},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B64*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$F64*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":0.20708333333333334},null,"Partikler (PM) (gram/liter)",{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B73*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$C73*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":0.29692643750000003},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B73*(1-'Vurdering af miljøgevinst'!$B$13)+Brændstoftyper!$F73*'Vurdering af miljøgevinst'!$B$13,\"IR\")","v":0.20190625000000001},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B73*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$C73*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":0.31062499999999998},{"$f":"IF('Vurdering af miljøgevinst'!$A$5=\"Rute 1\",Brændstoftyper!$B73*(1-'Vurdering af miljøgevinst'!$F$13)+Brændstoftyper!$F73*'Vurdering af miljøgevinst'!$F$13,\"IR\")","v":0.31062499999999998}]
[]
["Rute 2",null,null,null,null,"Rute 2","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 2","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 2","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 2","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 2","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 2","Kuldioxid (CO2) (gram/liter)"]
[null,null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)"]
[null,null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)"]
[null,null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)"]
[null,null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)"]
[null,null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)"]
[]
["Rute 3",null,null,null,null,"Rute 3","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 3","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 3","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 3","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 3","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 3","Kuldioxid (CO2) (gram/liter)"]
[null,null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)"]
[null,null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)"]
[null,null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)"]
[null,null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)"]
[null,null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)"]
[]
["Rute 4",null,null,null,null,"Rute 4","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 4","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 4","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 4","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 4","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 4","Kuldioxid (CO2) (gram/liter)"]
[null,null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)"]
[null,null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)"]
[null,null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)"]
[null,null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)"]
[null,null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)"]
[]
["Rute 5",null,null,null,null,"Rute 5","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 5","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 5","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 5","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 5","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 5","Kuldioxid (CO2) (gram/liter)"]
[null,null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)"]
[null,null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)"]
[null,null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)"]
[null,null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)"]
[null,null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)"]
[]
["Rute 6",null,null,null,null,"Rute 6","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 6","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 6","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 6","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 6","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 6","Kuldioxid (CO2) (gram/liter)"]
[null,null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)"]
[null,null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)"]
[null,null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)"]
[null,null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)"]
[null,null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)"]
[]
["Rute 7",null,null,null,null,"Rute 7","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 7","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 7","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 7","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 7","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 7","Kuldioxid (CO2) (gram/liter)"]
[null,null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)"]
[null,null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)"]
[null,null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)"]
[null,null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)"]
[null,null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)"]
[]
["Rute 8",null,null,null,null,"Rute 8","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 8","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 8","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 8","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 8","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 8","Kuldioxid (CO2) (gram/liter)"]
[null,null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)"]
[null,null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)"]
[null,null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)"]
[null,null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)"]
[null,null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)"]
[]
["Rute 9",null,null,null,null,"Rute 9","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 9","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 9","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 9","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 9","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 9","Kuldioxid (CO2) (gram/liter)"]
[null,null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)"]
[null,null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)"]
[null,null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)"]
[null,null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)"]
[null,null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)"]
[]
["Rute 10",null,null,null,null,"Rute 10","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 10","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 10","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 10","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 10","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 10","Kuldioxid (CO2) (gram/liter)"]
[null,null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)"]
[null,null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)"]
[null,null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)"]
[null,null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)"]
[null,null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)"]
[]
["Rute 11",null,null,null,null,"Rute 11","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 11","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 11","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 11","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 11","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 11","Kuldioxid (CO2) (gram/liter)"]
[null,null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)"]
[null,null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)"]
[null,null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)"]
[null,null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)"]
[null,null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)"]
[]
["Rute 12",null,null,null,null,"Rute 12","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 12","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 12","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 12","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 12","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 12","Kuldioxid (CO2) (gram/liter)"]
[null,null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)"]
[null,null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)"]
[null,null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)"]
[null,null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)"]
[null,null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)"]
[]
["Rute 13",null,null,null,null,"Rute 13","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 13","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 13","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 13","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 13","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 13","Kuldioxid (CO2) (gram/liter)"]
[null,null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)"]
[null,null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)"]
[null,null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)"]
[null,null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)"]
[null,null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)"]
[]
["Rute 14",null,null,null,null,"Rute 14","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 14","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 14","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 14","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 14","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 14","Kuldioxid (CO2) (gram/liter)"]
[null,null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)"]
[null,null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)"]
[null,null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)"]
[null,null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)"]
[null,null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)"]
[]
["Rute 15",null,null,null,null,"Rute 15","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 15","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 15","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 15","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 15","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 15","Kuldioxid (CO2) (gram/liter)"]
[null,null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)"]
[null,null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)"]
[null,null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)"]
[null,null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)"]
[null,null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)"]
[]
["Rute 16",null,null,null,null,"Rute 16","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 16","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 16","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 16","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 16","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 16","Kuldioxid (CO2) (gram/liter)"]
[null,null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)"]
[null,null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)"]
[null,null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)"]
[null,null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)"]
[null,null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)"]
[]
["Rute 17",null,null,null,null,"Rute 17","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 17","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 17","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 17","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 17","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 17","Kuldioxid (CO2) (gram/liter)"]
[null,null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)"]
[null,null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)"]
[null,null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)"]
[null,null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)"]
[null,null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)"]
[]
["Rute 18",null,null,null,null,"Rute 18","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 18","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 18","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 18","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 18","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 18","Kuldioxid (CO2) (gram/liter)"]
[null,null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)"]
[null,null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)"]
[null,null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)"]
[null,null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)"]
[null,null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)"]
[]
["Rute 19",null,null,null,null,"Rute 19","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 19","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 19","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 19","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 19","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 19","Kuldioxid (CO2) (gram/liter)"]
[null,null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)"]
[null,null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)"]
[null,null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)"]
[null,null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)"]
[null,null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)"]
[]
["Rute 20",null,null,null,null,"Rute 20","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 20","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 20","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 20","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 20","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 20","Kuldioxid (CO2) (gram/liter)"]
[null,null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)"]
[null,null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)"]
[null,null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)"]
[null,null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)"]
[null,null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)"]
[]
["Rute 21",null,null,null,null,"Rute 21","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 21","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 21","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 21","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 21","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 21","Kuldioxid (CO2) (gram/liter)"]
[null,null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)"]
[null,null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)"]
[null,null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)"]
[null,null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)"]
[null,null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)"]
[]
["Rute 22",null,null,null,null,"Rute 22","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 22","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 22","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 22","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 22","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 22","Kuldioxid (CO2) (gram/liter)"]
[null,null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)"]
[null,null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)"]
[null,null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)"]
[null,null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)"]
[null,null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)"]
[]
["Rute 23",null,null,null,null,"Rute 23","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 23","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 23","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 23","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 23","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 23","Kuldioxid (CO2) (gram/liter)"]
[null,null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)"]
[null,null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)"]
[null,null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)"]
[null,null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)"]
[null,null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)"]
[]
["Rute 24",null,null,null,null,"Rute 24","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 24","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 24","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 24","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 24","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 24","Kuldioxid (CO2) (gram/liter)"]
[null,null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)"]
[null,null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)"]
[null,null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)"]
[null,null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)"]
[null,null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)"]
[]
["Rute 25",null,null,null,null,"Rute 25","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 25","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 25","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 25","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 25","Kuldioxid (CO2) (gram/liter)",null,null,null,null,"Rute 25","Kuldioxid (CO2) (gram/liter)"]
[null,null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)",null,null,null,null,null,"Svovldioxid (SO2) (gram/liter)"]
[null,null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)",null,null,null,null,null,"Kvælstofilter (NOx) (gram/liter)"]
[null,null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)",null,null,null,null,null,"Kulilte (CO) (gram/liter)"]
[null,null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)",null,null,null,null,null,"Kulbrinte (HC) (gram/liter)"]
[null,null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)",null,null,null,null,null,"Partikler (PM) (gram/liter)"]